{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Start","Part number search","SO-Products"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Start","index":0,"n_rows":33,"n_cols":13,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[null,null,"Smartoptics Transceiver Search Tool"]
[]
[null,null,null,"Update date: ",null,null,"August 5, 2022",null,null,null,null,null,"Note! "]
[null,null,null,"Revision:",null,null,14,null,null,null,null,null,"There are frequent additions of new transceivers and also"]
[null,null,null,null,null,null,null,null,null,null,null,null,"updates in datasheets. Please check for more recent versions  "]
[null,null,null,null,null,null,null,null,null,null,null,null,"of this tool at regular intervals. "]
[]
[]
[null,null,"Introduction/Instruction"]
[]
[null,null,null,"This tool contains two sections/tabs:"]
[]
[null,null,null,"Part number search: Enter a SO part number and see selected data."]
[]
[null,null,null,"SO-Products: Via radio-buttons in the upper left side, one can select attributes to filter out and narrow down the alternatives. "]
[null,null,null,"Attributes not available via radio-buttons can (if needed) give further filtering via the arrows in the column headings. "]
[]
[null,null,null,"The far right column provides a link to the corresponding datasheet located on the external Smartoptics web site. "]
[]
[null,null,null,"The button\"Reset Filters\" clears all filtering settings."]
[]
[]
[]
[]
[]
[null,"Smartoptics makes no warranties or representations, expressed or implied, of any kind relative to the information or any portion thereof contained in this document or its adaptation or use, and assumes no "]
[null,"responsibility or liability of any kind, including, but not limited to, indirect, special, consequential or incidental damages, for any errors or inaccuracies contained in the information or arising from the adaptation  "]
[null,"or use of the information or any portion thereof. The information in this document is subject to change without notice."]

{"sheet":"Part number search","index":1,"n_rows":15,"n_cols":55,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,null,null,null,"Part number:  ","TQ2023-S31C-SO",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[]
[]
[]
[null,null,null,"Form-factor:",null,{"$f":"_xlfn.IFNA(VLOOKUP(F4,Table2[[Part number]:[Temp]],3,FALSE),\"P/N Does not exist\")","v":"QSFP28"}]
[]
[null,null,null,"Description:",null,{"$f":"_xlfn.IFNA(VLOOKUP(F4,Table2[[Part number]:[Temp]],2,FALSE),\"P/N Does not exist\")","v":"QSFP28, 100G Ethernet ER1, SM 1x 1310nm, 40km, 18.5dB, LC"}]
[]
[null,null,null,"Technology:",null,{"$f":"_xlfn.IFNA(VLOOKUP(F4,Table2[[Part number]:[Temp]],4,FALSE),\"P/N Does not exist\")","v":"Grey"}]
[]
[null,null,null,"Protocol support:",null,{"$f":"_xlfn.IFNA(VLOOKUP(F4,Table2[[Part number]:[Temp]],8,FALSE),\"P/N Does not exist\")","v":"100GE"}]

{"sheet":"SO-Products","index":2,"n_rows":2381,"n_cols":31,"rows_kept":2381,"cut":false,"hidden":false,"merged":[]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FormFactor","Techn","Media","Fiber","Protocol"]
[null,"SO Transceivers with selected attributes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,7,5,1,7]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,7,5,1,7]
[]
[null,null,null,null,null,"Select attributes via the radio buttons. Use the extra filtering functionality in the tabel headings if required."]
[null,null,null,null,null,"The table is not protected, so do not change the content."]
[null,null,null,null,null,"More detailed information can be found via the datasheet that can be downloaded via the links. "]
[]
[]
[]
[]
[null,"Part number","Description","Form-factor","Technology","Media Type","Fiber","Wavelengths","Protocols","Distance","MSA/Std","Temp","Datasheet"]
[null,"SO-CFP-40GBase-LR4","CFP, 40G Ethernet LR4, SDH/SONET, OTN, SM 1271/1291/1311/1331nm, 10km, 6.7dB, LC","CFP","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","40GE","10km","40GBASE-LR4","C-temp","Datasheet"]
[null,"SO-CFP-40GBase-LR4-20","CFP, 40G Ethernet LR4, SM 1271/1291/1311/1331nm, 20km, 10.7dB, LC","CFP","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","40GE","20km","40GBASE-LR4","C-temp","Datasheet"]
[null,"SO-CFP-ER4","CFP, 100G Ethernet ER4, OTU4, SM 1296/1300/1305/1309nm, 40km, 18dB, LC","CFP","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE/OTU4","40km","100GBASE-ER4","C-temp","Datasheet"]
[null,"SO-CFP-LR4","CFP, 100G Ethernet LR4, OTU4, SM 1296/1300/1305/1309nm, 10km, 6.3dB, LC","CFP","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE/OTU4","10km","100GBASE-LR4","C-temp","Datasheet"]
[null,"SO-CFP-SR10","CFP, 100G Ethernet SR10, MM 10x 850nm, 100m, 1.8dB, MPO","CFP","Grey","Ribbon","MM","10x 850nm","100GE","100m","100GBASE-SR10","C-temp","Datasheet"]
[null,"SO-CFP2-ER4","CFP2, 100G Ethernet ER4, OTU4, SM 1296/1300/1305/1309nm, 40km, 18dB, LC","CFP2","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE/OTU4","40km","100GBASE-ER4","C-temp","Datasheet"]
[null,"SO-CFP2-LR4","CFP2, 100G Ethernet LR4, OTU4, SM 1296/1300/1305/1309nm, 10km, 6.3dB, LC","CFP2","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE/OTU4","10km","100GBASE-LR4","C-temp","Datasheet"]
[null,"SO-CFP2-QSFP28-1M","CFP2 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, OTU4, AWG30, 1m","CFP2/QSFP28","DAC","Coax","Electrical","-","100GE/OTU4","1m","-","C-temp","Datasheet"]
[null,"SO-CFP2-QSFP28-2M","CFP2 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, OTU4, AWG30, 2m","CFP2/QSFP28","DAC","Coax","Electrical","-","100GE/OTU4","2m","-","C-temp","Datasheet"]
[null,"SO-CFP2-QSFP28-3M","CFP2 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, OTU4, AWG30, 3m","CFP2/QSFP28","DAC","Coax","Electrical","-","100GE/OTU4","3m","-","C-temp","Datasheet"]
[null,"SO-CFP2-QSFP28-1M-2","CFP2 to QSFP28 Direct Attach Cable (DAC), Dual CDR, 100G Ethernet, OTU4, AWG30, 1m","CFP2/QSFP28","DAC","Coax","Electrical","-","100GE/OTU4","1m","-","C-temp","Datasheet"]
[null,"SO-CFP2-QSFP28-2M-2","CFP2 to QSFP28 Direct Attach Cable (DAC), Dual CDR, 100G Ethernet, OTU4, AWG30, 2m","CFP2/QSFP28","DAC","Coax","Electrical","-","100GE/OTU4","2m","-","C-temp","Datasheet"]
[null,"SO-CFP2-QSFP28-3M-2","CFP2 to QSFP28 Direct Attach Cable (DAC), Dual CDR, 100G Ethernet, OTU4, AWG30, 3m","CFP2/QSFP28","DAC","Coax","Electrical","-","100GE/OTU4","3m","-","C-temp","Datasheet"]
[null,"SO-CFP4-LR4","CFP4, 100G Ethernet LR4, OTU4, SM 1296/1300/1305/1309nm, 10km, 6.3dB, LC","CFP4","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE/OTU4","10km","100GBASE-LR4","C-temp","Datasheet"]
[null,"SO-CFP4-SR4","CFP4, 100G Ethernet SR4, MM 4x 850nm, 100m, 1.9dB, MPO","CFP4","Grey","Ribbon","MM","4x 850nm","100GE","100m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-CFP-LPC-DWDM","CFP-DCO Low Tx Power, 100G Eth, DWDM 6,25/50GHz Coh, 191.25-196.10THz, 2400km, 25dB, LC","CFP-DCO","DWDM/50GHz-Tune","Fiber-pair","SM","D9125-D9610","100GE","2400km","-","C-temp","Datasheet"]
[null,"SO-CSFP-1000Base-BX10D-43-O2","CSFP, BiDi, Multirate 100Mbps - 1.25Gbps, TX/RX=1490/1310nm, SM, 10km, 11dB, LC","CSFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC/STM-4/OC-12/STM-1/OC-3","10km","-","C-temp","Datasheet"]
[null,"SO-CSFP-1000Base-BX10D-43-O2-I","CSFP, BiDi, Multirate 100Mbps - 1.25Gbps, TX/RX=1490/1310nm, SM, 10km, 11dB, I-temp, LC","CSFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC/STM-4/OC-12/STM-1/OC-3","10km","-","I-temp","Datasheet"]
[null,"SO-CSFP-1000Base-BX10D-53-O2","CSFP, BiDi, Multirate 100Mbps - 1.25Gbps, TX/RX=1550/1310nm, SM, 10km, 11dB, LC","CSFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/FE/1G FC/STM-4/OC-12/STM-1/OC-3","10km","-","C-temp","Datasheet"]
[null,"SO-CSFP-1000Base-BX10D-53-O2-I","CSFP, BiDi, Multirate 100Mbps - 1.25Gbps, TX/RX=1550/1310nm, SM, 10km, 11dB, I-temp, LC","CSFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/FE/1G FC/STM-4/OC-12/STM-1/OC-3","10km","-","I-temp","Datasheet"]
[null,"SO-CSFP-1000Base-BX20D-43-O2","CSFP, BiDi, Multirate 100Mbps - 1.25Gbps, TX/RX=1490/1310nm, SM, 20km, 14dB, LC","CSFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC/STM-4/OC-12/STM-1/OC-3","20km","-","C-temp","Datasheet"]
[null,"SO-CSFP-1000Base-BX20D-43-O2-I","CSFP, BiDi, Multirate 100Mbps - 1.25Gbps, TX/RX=1490/1310nm, SM, 20km, 14dB, I-temp, LC","CSFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC/STM-4/OC-12/STM-1/OC-3","20km","-","I-temp","Datasheet"]
[null,"SO-CSFP-1000Base-BX20D-53-O2","CSFP, BiDi, Multirate 100Mbps - 1.25Gbps, TX/RX=1550/1310nm, SM, 20km, 14dB, LC","CSFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/FE/1G FC/STM-4/OC-12/STM-1/OC-3","20km","-","C-temp","Datasheet"]
[null,"SO-CSFP-1000Base-BX20D-53-O2-I","CSFP, BiDi, Multirate 100Mbps - 1.25Gbps, TX/RX=1550/1310nm, SM, 20km, 14dB, I-temp, LC","CSFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/FE/1G FC/STM-4/OC-12/STM-1/OC-3","20km","-","I-temp","Datasheet"]
[null,"SO-QSFP-4SFP-ACU3M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG30, 3m, active","QSFP+","DAC","Coax","Electrical","-","40GE","3m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-ACU5M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG30, 5m, active","QSFP+","DAC","Coax","Electrical","-","40GE","5m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-ACU7M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG30, 7m, active","QSFP+","DAC","Coax","Electrical","-","40GE","7m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-ACU10M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG26, 10m, active","QSFP+","DAC","Coax","Electrical","-","40GE","10m","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC1M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 1m","QSFP+","AOC","Ribbon","MM","850nm","40GE","1m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC2M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 2m","QSFP+","AOC","Ribbon","MM","850nm","40GE","2m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC3M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 3m","QSFP+","AOC","Ribbon","MM","850nm","40GE","3m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC4M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 4m","QSFP+","AOC","Ribbon","MM","850nm","40GE","4m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC5M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 5m","QSFP+","AOC","Ribbon","MM","850nm","40GE","5m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC6M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 6m","QSFP+","AOC","Ribbon","MM","850nm","40GE","6m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC7M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 7m","QSFP+","AOC","Ribbon","MM","850nm","40GE","7m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC8M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 8m","QSFP+","AOC","Ribbon","MM","850nm","40GE","8m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC9M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 9m","QSFP+","AOC","Ribbon","MM","850nm","40GE","9m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC10M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 10m","QSFP+","AOC","Ribbon","MM","850nm","40GE","10m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC15M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 15m","QSFP+","AOC","Ribbon","MM","850nm","40GE","15m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC20M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 20m","QSFP+","AOC","Ribbon","MM","850nm","40GE","20m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC30M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 30m","QSFP+","AOC","Ribbon","MM","850nm","40GE","30m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC50M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 50m","QSFP+","AOC","Ribbon","MM","850nm","40GE","50m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-AOC100M","QSFP+, Active Optical Cable (AOC), 40G Ethernet, 100m","QSFP+","AOC","Ribbon","MM","850nm","40GE","100m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-PCU1M","QSFP+ to QSFP+, Direct Attach Cable (DAC), 40G Ethernet, AWG30, 1m, passive","QSFP+","DAC","Coax","Electrical","-","40GE","1m","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-PCU2M","QSFP+ to QSFP+, Direct Attach Cable (DAC), 40G Ethernet, AWG30, 2m, passive","QSFP+","DAC","Coax","Electrical","-","40GE","2m","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-PCU3M","QSFP+ to QSFP+, Direct Attach Cable (DAC), 40G Ethernet, AWG28, 3m, passive","QSFP+","DAC","Coax","Electrical","-","40GE","3m","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-PCU5M","QSFP+ to QSFP+, Direct Attach Cable (DAC), 40G Ethernet, AWG26, 5m, passive","QSFP+","DAC","Coax","Electrical","-","40GE","5m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D20","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9200","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9200","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D21","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9210","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9210","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D22","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9220","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9220","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D23","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9230","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9230","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D24","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9240","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9240","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D25","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9250","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9250","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D26","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9260","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9260","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D27","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9270","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9270","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D28","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9280","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9280","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D29","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9290","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9290","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D30","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9300","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9300","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D31","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9310","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9310","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D32","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9320","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9320","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D33","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9330","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9330","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D34","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9340","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9340","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D35","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9350","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9350","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D36","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9360","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9360","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D37","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9370","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9370","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D38","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9380","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9380","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D39","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9390","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9390","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D40","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9400","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9400","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D41","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9410","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9410","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D42","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9420","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9420","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D43","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9430","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9430","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D44","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9440","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9440","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D45","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9450","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9450","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D46","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9460","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9460","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D47","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9470","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9470","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D48","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9480","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9480","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D49","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9490","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9490","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D50","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9500","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9500","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D51","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9510","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9510","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D52","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9520","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9520","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D53","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9530","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9530","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D54","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9540","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9540","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D55","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9550","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9550","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D56","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9560","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9560","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D57","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9570","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9570","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D58","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9580","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9580","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D59","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D9590","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9590","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D20-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D920 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9200","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D21-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D921 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9210","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D22-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D922 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9220","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D23-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D923 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9230","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D24-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D924 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9240","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D25-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D925 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9250","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D26-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D926 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9260","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D27-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D927 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9270","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D28-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D928 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9280","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D29-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D929 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9290","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D30-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D930 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9300","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D31-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D931 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9310","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D32-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D932 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9320","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D33-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D933 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9330","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D34-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D934 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9340","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D35-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D935 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9350","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D36-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D936 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9360","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D37-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D937 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9370","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D38-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D938 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9380","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D39-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D939 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9390","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D40-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D940 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9400","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D41-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D941 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9410","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D42-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D942 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9420","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D43-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D943 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9430","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D44-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D944 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9440","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D45-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D945 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9450","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D46-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D946 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9460","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D47-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D947 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9470","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D48-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D948 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9480","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D49-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D949 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9490","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D50-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D950 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9500","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D51-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D951 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9510","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D52-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D952 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9520","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D53-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D953 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9530","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D54-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D954 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9540","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D55-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D955 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9550","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D56-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D956 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9560","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D57-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D957 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9570","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D58-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D958 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9580","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D59-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D959 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM"," D9590","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP28-D60-A","QSFP28, 100G Eth, PAM4, DWDM 100GHz, LC, D960 A-version","QSFP28","DWDM/100GHz","Fiber-pair","SM","D9600","100GE","See datasheet","-","C-temp","Datasheet"]
[null,"SO-QSFP-ER4","QSFP+, 40G Ethernet ER4, SM, 1271/1291/1311/1331nm, 40km, 18.5dB, LC","QSFP+","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","40GE/OTU3","40km","40GBASE-ER4","C-temp","Datasheet"]
[null,"SO-QSFP-IR4-PSM","QSFP+, 40G Ethernet IR4, SM, 1310nm, 2km, 7.4dB, MPO (APC)","QSFP+","Grey","Ribbon","SM","4x 1310nm","40GE","2km","40GBASE-IR4","C-temp","Datasheet"]
[null,"SO-QSFP-LR4","QSFP+, 40G Ethernet LR4, OTU3, SM, 1271/1291/1311/1331nm, 10km, 6.7dB, LC","QSFP+","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","40GE/OTU3","10km","40GBASE-LR4","C-temp","Datasheet"]
[null,"SO-QSFP-LR4-20","QSFP+, 40G Ethernet LR4, SM, 1271/1291/1311/1331nm, 20km, 10.2dB, LC","QSFP+","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","40GE","20km","40GBASE-LR4","C-temp","Datasheet"]
[null,"SO-QSFP-LR4-PSM","QSFP+, 40G Ethernet LR4, SM, 1310nm, 10km, 6.6dB, MPO (APC)","QSFP+","Grey","Fiber-pair","SM","4x 1310nm","40GE/10GbE-LAN","10km","40GBASE-LR4","C-temp","Datasheet"]
[null,"SO-QSFP-LX4","QSFP+, 40G Ethernet IR4, 1271/1291/1311/1331nm, 2km@SM, 150m@OM3, 300m@OM4, 4.5dB, LC","QSFP+","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","40GE","2km","40GBASE-IR4","C-temp","Datasheet"]
[null,"SO-QSFP-LX4","QSFP+, 40G Ethernet IR4, 1271/1291/1311/1331nm, 2km@SM, 150m@OM3, 300m@OM4, 4.5dB, LC","QSFP+","Grey","Fiber-pair","MM","1271/1291/1311/1331nm","40GE","150m/300m","40GBASE-IR4","C-temp","Datasheet"]
[null,"SO-QSFP-SR4","QSFP+, 40G Ethernet SR4, MM 850nm, 150m@OM4, 4.5dB, MPO","QSFP+","Grey","Ribbon","MM","4x 850nm","40GE/10GbE-LAN","150m","40GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP-ESR4","QSFP+, 40G Ethernet eSR4, MM 850nm, 300m/OM3, 400m/OM4, 1.9dB, MPO","QSFP+","Grey","Ribbon","MM","4x 850nm","40GE","400m","40GBASE-eSR4","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9210","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9210","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9210","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9220","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9220","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9220","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9230","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9230","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9230","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9240","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9240","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9240","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9250","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9250","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9250","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9260","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9260","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9260","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9270","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9270","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9270","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9280","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9280","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9280","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9290","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9290","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9290","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9300","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9300","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9300","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9310","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9310","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9310","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9320","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9320","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9320","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9330","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9330","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9330","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9340","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9340","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9340","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9350","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9350","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9350","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9360","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9360","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9360","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9370","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9370","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9370","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9380","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9380","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9380","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9390","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9390","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9390","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9400","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9400","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9400","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9410","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9410","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9410","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9420","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9420","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9420","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9430","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9430","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9430","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9440","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9440","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9440","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9450","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9450","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9450","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9460","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9460","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9460","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9470","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9470","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9470","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9480","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9480","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9480","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9490","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9490","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9490","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9500","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9500","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9500","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9510","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9510","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9510","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9520","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9520","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9520","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9530","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9530","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9530","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9540","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9540","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9540","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9550","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9550","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9550","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9560","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9560","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9560","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9570","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9570","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9570","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9580","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9580","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9580","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9590","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9590","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9590","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-40G-D9600","QSFP+ 40G Ethernet DWDM 100GHz 8km 10dB LC D9600","QSFP+","DWDM/100GHz","Fiber-pair","SM"," D9600","40GE","8km","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-ACU3M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG30, 3m, active","QSFP+/SFP+","DAC","Coax","Electrical","-","40GE/10GbE-LAN","3m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-ACU5M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG30, 5m, active","QSFP+/SFP+","DAC","Coax","Electrical","-","40GE/10GbE-LAN","5m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-ACU7M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG30, 7m, active","QSFP+/SFP+","DAC","Coax","Electrical","-","40GE/10GbE-LAN","7m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-ACU10M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG26, 10m, active","QSFP+/SFP+","DAC","Coax","Electrical","-","40GE/10GbE-LAN","10m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-PCU1M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG30, 1m, passive","QSFP+/SFP+","DAC","Coax","Electrical","-","40GE/10GbE-LAN","1m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-PCU2M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG30, 2m, passive","QSFP+/SFP+","DAC","Coax","Electrical","-","40GE/10GbE-LAN","2m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-PCU3M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG30, 3m, passive","QSFP+/SFP+","DAC","Coax","Electrical","-","40GE/10GbE-LAN","3m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4SFP-PCU5M","QSFP+ to 4xSFP+, Direct Attach Cable (DAC), 40G to 10G Eth, AWG26, 5m, passive","QSFP+/SFP+","DAC","Coax","Electrical","-","40GE/10GbE-LAN","5m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC1M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 1m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","1m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC2M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 2m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","2m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC3M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 3m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","3m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC4M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 4m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","4m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC5M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 5m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","5m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC6M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 6m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","6m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC7M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 7m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","7m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC8M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 8m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","8m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC9M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 9m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","9m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC10M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 10m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","10m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC15M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 15m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","15m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC20M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 20m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","20m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC30M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 30m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","30m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC50M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 50m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","50m","-","C-temp","Datasheet"]
[null,"SO-QSFP-4X10G-AOC100M","QSFP+ to 4xSFP+, Active Optical Cable (AOC), 40G to 10G Ethernet, 100m","QSFP+/SFP+","AOC","Fiber-pair","MM",null,"40GE/10GbE-LAN","100m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-DR","QSFP28 100G Ethernet DR SM 1x 1311nm PAM4 500m 3dB LC","QSFP28","Grey","Fiber-pair","SM","1311nm","100GE","500m","100G-DR","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-FR","QSFP28 100G Ethernet FR SM 1x 1311nm PAM4 2km 4dB LC","QSFP28","Grey","Fiber-pair","SM","1311nm","100GE","2km","100G-FR","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-FRA","QSFP28 100G Ethernet FR SM 1x 1271nm PAM4 2km 4dB LC","QSFP28","Grey","Fiber-pair","SM","1271nm","100GE","2km","100G-FR","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-FRB","QSFP28 100G Ethernet FR SM 1x 1291nm PAM4 2km 4dB LC","QSFP28","Grey","Fiber-pair","SM","1291nm","100GE","2km","100G-FR","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-FRC","QSFP28 100G Ethernet FR SM 1x 1311nm PAM4 2km 4dB LC","QSFP28","Grey","Fiber-pair","SM","1311nm","100GE","2km","100G-FR","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-FRD","QSFP28 100G Ethernet FR SM 1x 1331nm PAM4 2km 4dB LC","QSFP28","Grey","Fiber-pair","SM","1331nm","100GE","2km","100G-FR","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-LR","QSFP28 100G Ethernet LR SM 1x 1311nm PAM4 10km 6.3dB LC","QSFP28","Grey","Fiber-pair","SM","1311nm","100GE","10km","100G-LR","C-temp","Datasheet"]
[null,"TQ2023-S31C-SO","QSFP28, 100G Ethernet ER1, SM 1x 1310nm, 40km, 18.5dB, LC","QSFP28","Grey","Fiber-pair","SM","1311nm","100GE","40km","100G ER1-40","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-LRA","QSFP28 100G Ethernet LR SM 1x 1271nm PAM4 10km 6.3dB LC","QSFP28","Grey","Fiber-pair","SM","1271nm","100GE","10km","100G-LR","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-LRB","QSFP28 100G Ethernet LR SM 1x 1291nm PAM4 10km 6.3dB LC","QSFP28","Grey","Fiber-pair","SM","1291nm","100GE","10km","100G-LR","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-LRC","QSFP28 100G Ethernet LR SM 1x 1311nm PAM4 10km 6.3dB LC","QSFP28","Grey","Fiber-pair","SM","1311nm","100GE","10km","100G-LR","C-temp","Datasheet"]
[null,"SO-QSFP28-100G-LRD","QSFP28 100G Ethernet LR SM 1x 1331nm PAM4 10km 6.3dB LC","QSFP28","Grey","Fiber-pair","SM","1331nm","100GE","10km","100G-LR","C-temp","Datasheet"]
[null,"TQ2020-BADC-SO","QSFP28, BiDi, 100G Eth, Tx/Rx=1271/1331nm, SM, 10km, 6.8dB, LC","QSFP28","Grey","Fiber-pair","SM","1271/1331nm","100GE","10km","100G-LR","C-temp","Datasheet"]
[null,"TQ2020-BDAC-SO","QSFP28, BiDi, 100G Eth, Tx/Rx=1331/1271nm, SM, 10km, 6.8dB, LC","QSFP28","Grey","Fiber-pair","SM","1271/1331nm","100GE","10km","100G-LR","C-temp","Datasheet"]
[null,"TQ2021-BBCC-SO","QSFP28, BiDi, 100G Eth, Tx/Rx=1291/1311nm, SM, 20km, 10.4dB, LC","QSFP28","Grey","Fiber-pair","SM","1291/1311nm","100GE","20km","100G LR1-20","C-temp","Datasheet"]
[null,"TQ2021-BCBC-SO","QSFP28, BiDi, 100G Eth, Tx/Rx=1311/1291nm, SM, 20km, 10.4dB, LC","QSFP28","Grey","Fiber-pair","SM","1291/1311nm","100GE","20km","100G LR1-20","C-temp","Datasheet"]
[null,"SO-QSFP28-50GE-BX10D-2733","QSFP28, BiDi, 50G Ethernet, Tx/Rx=1270/1330nm, SM, 10km, 6.3dB, LC","QSFP28","BiDi","Single-fiber","SM","1270/1330nm","50GE","10km","-","C-temp","Datasheet"]
[null,"SO-QSFP28-50GE-BX10D-3327","QSFP28, BiDi, 50G Ethernet, Tx/Rx=1330/1270nm, SM, 10km, 6.3dB, LC","QSFP28","BiDi","Single-fiber","SM","1270/1330nm","50GE","10km","-","C-temp","Datasheet"]
[null,"SO-QSFP28-50GE-BX40D-2930","QSFP28, BiDi, 50G Ethernet, Tx/Rx=1294.40nm/1308.24nm, SM, 40km, 18dB, LC","QSFP28","BiDi","Single-fiber","SM","1294.40nm/1308.24nm","50GE","40km","-","C-temp","Datasheet"]
[null,"SO-QSFP28-50GE-BX40D-3029","QSFP28, BiDi, 50G Ethernet, Tx/Rx=1308.24nm/1294.40nm, SM, 40km, 18dB, LC","QSFP28","BiDi","Single-fiber","SM","1294.40nm/1308.24nm","50GE","40km","-","C-temp","Datasheet"]
[null,"SO-QSFP28-ZR4","QSFP28, 100G Ethernet ZR4, SM 1296/1300/1305/1309nm, 80km, 31dB, LC","QSFP28","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE","80km","100G-ZR4","C-temp","Datasheet"]
[null,"QSFP-100G-ZR4-SO","QSFP28, 100G Ethernet ZR4, SM 1296/1300/1305/1309nm, 80km, 31dB, for CISCO in \"unsupported\" mode, LC","QSFP28","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE","80km","100G-ZR4","C-temp","Datasheet"]
[null,"SO-SFP28-LWDM-A-E","SFP28 25GE CPRI opt 10 LANWDM 1295.56nm SM DDM 21dB 30km, E-temp, LC","SFP28","LANWDM","Fiber-pair","SM","1295.56nm","25GE/CPRI-10","30km","-","E-temp","Datasheet"]
[null,"SO-SFP28-LWDM-B-E","SFP28 25GE CPRI opt 10 LANWDM 1300.05nm SM DDM 21dB 30km, E-temp, LC","SFP28","LANWDM","Fiber-pair","SM","1300.05nm","25GE/CPRI-10","30km","-","E-temp","Datasheet"]
[null,"SO-SFP28-LWDM-C-E","SFP28 25GE CPRI opt 10 LANWDM 1304.58nm SM DDM 21dB 30km, E-temp, LC","SFP28","LANWDM","Fiber-pair","SM","1304.58nm","25GE/CPRI-10","30km","-","E-temp","Datasheet"]
[null,"SO-SFP28-LWDM-D-E","SFP28 25GE CPRI opt 10 LANWDM 1309.14nm SM DDM 21dB 30km, E-temp, LC","SFP28","LANWDM","Fiber-pair","SM","1309.14nm","25GE/CPRI-10","30km","-","E-temp","Datasheet"]
[null,"SO-SFP28-LWDM-E-E","SFP28 25GE CPRI opt 10 LANWDM 1277.89nm SM DDM 21dB 30km, E-temp, LC","SFP28","LANWDM","Fiber-pair","SM","1277.89nm","25GE/CPRI-10","30km","-","E-temp","Datasheet"]
[null,"SO-SFP28-LWDM-F-E","SFP28 25GE CPRI opt 10 LANWDM 1282.26nm SM DDM 21dB 30km, E-temp, LC","SFP28","LANWDM","Fiber-pair","SM","1282.26nm","25GE/CPRI-10","30km","-","E-temp","Datasheet"]
[null,"SO-SFP28-LWDM-G-E","SFP28 25GE CPRI opt 10 LANWDM 1286.66nm SM DDM 21dB 30km, E-temp, LC","SFP28","LANWDM","Fiber-pair","SM","1286.66nm","25GE/CPRI-10","30km","-","E-temp","Datasheet"]
[null,"SO-SFP28-LWDM-H-E","SFP28 25GE CPRI opt 10 LANWDM 1291.10nm SM DDM 21dB 30km, E-temp, LC","SFP28","LANWDM","Fiber-pair","SM","1291.10nm","25GE/CPRI-10","30km","-","E-temp","Datasheet"]
[null,"SO-SFP28-L10-D9200-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9200","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9200","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9210-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9210","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9210","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9220-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9220","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9220","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9230-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9230","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9230","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9240-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9240","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9240","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9250-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9250","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9250","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9260-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9260","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9260","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9270-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9270","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9270","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9280-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9280","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9280","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9290-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9290","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9290","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9300-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9300","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9300","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9310-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9310","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9310","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9320-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9320","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9320","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9330-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9330","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9330","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9340-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9340","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9340","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9350-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9350","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9350","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9360-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9360","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9360","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9370-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9370","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9370","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9380-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9380","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9380","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9390-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9390","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9390","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9400-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9400","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9400","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9410-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9410","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9410","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9420-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9420","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9420","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9430-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9430","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9430","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9440-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9440","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9440","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9450-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9450","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9450","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9460-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9460","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9460","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9470-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9470","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9470","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9480-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9480","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9480","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9490-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9490","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9490","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9500-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9500","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9500","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9510-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9510","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9510","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9520-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9520","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9520","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9530-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9530","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9530","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9540-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9540","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9540","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9550-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9550","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9550","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9560-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9560","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9560","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9570-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9570","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9570","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9580-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9580","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9580","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9590-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9590","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9590","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10-D9600-I","SFP28 25G Ethernet DWDM 10km 13dB I-temp LC D9600","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9600","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9200-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9200","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9200","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9210-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9210","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9210","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9220-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9220","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9220","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9230-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9230","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9230","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9240-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9240","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9240","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9250-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9250","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9250","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9260-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9260","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9260","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9270-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9270","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9270","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9280-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9280","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9280","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9290-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9290","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9290","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9300-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9300","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9300","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9310-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9310","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9310","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9320-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9320","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9320","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9330-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9330","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9330","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9340-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9340","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9340","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9350-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9350","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9350","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9360-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9360","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9360","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9370-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9370","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9370","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9380-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9380","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9380","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9390-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9390","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9390","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9400-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9400","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9400","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9410-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9410","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9410","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9420-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9420","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9420","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9430-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9430","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9430","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9440-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9440","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9440","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9450-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9450","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9450","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9460-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9460","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9460","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9470-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9470","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9470","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9480-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9480","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9480","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9490-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9490","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9490","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9500-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9500","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9500","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9510-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9510","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9510","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9520-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9520","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9520","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9530-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9530","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9530","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9540-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9540","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9540","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9550-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9550","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9550","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9560-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9560","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9560","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9570-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9570","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9570","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9580-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9580","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9580","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9590-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9590","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9590","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-L10E-D9600-I","SFP28 25G Ethernet DWDM 10km 18dB I-temp LC D9600","SFP28","DWDM/100GHz","Fiber-pair","SM"," D9600","25GE/CPRI-10","10km","-","I-temp","Datasheet"]
[null,"SO-SFP28-32GFC-SD","SFP28, 32G FC, 25G Ethernet, MM, 850nm, 100m@OM4, 7dB, LC","SFP28","Grey","Fiber-pair","MM","850nm","32G_FC/25GE","100m","-","C-temp","Datasheet"]
[null,"SO-SFP28-32GFC-LD","SFP28, 32G/16G/8G FC, 25G Ethernet, SM, 1310nm, 10km, 9.4dB, LC","SFP28","Grey","Fiber-pair","SM","1310nm","32G_FC/25GE","10km","-","C-temp","Datasheet"]
[null,"SO-QSFP-DD-4C-DR4-M","QSFP-DD 400G-DR4 Ethernet, 4x100G-DR PAM4 CMIS3.0, 4x 1311nm 500m 3dB MPO12","QSFP-DD","Grey","Ribbon","SM","4x 1311nm","400GE","500m","400G-DR4","C-temp","Datasheet"]
[null,"SO-QSFP-DD-4C-DR4-4-M","QSFP-DD 400G-DR4 Ethernet, 4x100G-DR PAM4 CMIS4.0, 4x 1311nm 500m 3dB MPO12","QSFP-DD","Grey","Ribbon","SM","4x 1311nm","400GE","500m","400G-DR4","C-temp","Datasheet"]
[null,"SO-QSFP-DD-4C-FR4","QSFP-DD 400G-FR4 Ethernet, 4×100G-FR, PAM4 CMIS3.0, 1271nm/1291nm/1311nm/1331nm 2km 4dB LC","QSFP-DD","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","400GE","2km","400G-FR4","C-temp","Datasheet"]
[null,"SO-QSFP-DD-4C-FR4-4","QSFP-DD 400G-FR4 Ethernet, 4×100G-FR, PAM4 CMIS4.0, 1271nm/1291nm/1311nm/1331nm 2km 4dB LC","QSFP-DD","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","400GE","2km","400G-FR4","C-temp","Datasheet"]
[null,"SO-QSFP-DD-4C-LR4","QSFP-DD 400G-LR4 Ethernet, 4x100G-LR, PAM4 CMIS3.0, 1271nm/1291nm/1311nm/1331nm 10km 6.3dB LC","QSFP-DD","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","400GE","10km","400G-LR4","C-temp","Datasheet"]
[null,"SO-QSFP-DD-4C-LR4-4","QSFP-DD 400G-LR4 Ethernet, 4x100G-LR, PAM4 CMIS4.0, 1271nm/1291nm/1311nm/1331nm 10km 6.3dB LC","QSFP-DD","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","400GE","10km","400G-LR4","C-temp","Datasheet"]
[null,"SO-TQSFP-DD-4CC-ZR","QSFP-DD OIF 400GZR Ethernet Coh Tunable Flexgrid 120km LC","QSFP-DD","DWDM/50GHz","Fiber-pair","SM","D9128 - D9612","400GE","120km","OIF400ZR","C-temp","Datasheet"]
[null,"SO-TQSFPDD4CCZRP","QSFP-DD OIF400G/OpenZR+ Coh Tunable Flexgrid, LC","QSFP-DD","DWDM/50GHz","Fiber-pair","SM","D9128 - D9612","400GE/100GE","120km","OpenZR+","C-temp","Datasheet"]
[null,"TQD011-TUNC-SO","QSFP-DD 100G Coherent Tunable SM 450km CMIS4.1 LC","QSFP-DD","DWDM/50GHz","Fiber-pair","SM","D9128 - D9612","100GE","450km","OpenZR+","C-temp","Datasheet"]
[null,"SO-QSFP-DD-2C-10","QSFP-DD 2x100G Ethernet-LR4 10km, 1296/1300/1305/1309nm, 7.3dB CMIS3 Dual CS","QSFP-DD","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE","10km","100G-LR4","C-temp","Datasheet"]
[null,"SO-QSFP-DD-2C-10-4","QSFP-DD 2x100G Ethernet-LR4 10km, 1296/1300/1305/1309nm, 7.3dB CMIS4 Dual CS","QSFP-DD","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE","10km","100G-LR4","C-temp","Datasheet"]
[null,"SO-QSFP56-2C-2","QSFP56 200G-FR4 Ethernet, 1271nm/1311nm/1311nm/1331nm, 2km, 4.8dB, CMIS4.0, LC","QSFP56","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","200GE","2km","200G-FR4","C-temp","Datasheet"]
[null,"SO-QDD-4C-0CU5-4","QSFP-DD Active Electrical Cable (AEC) 400G Ethernet, AWG32, CMIS4, 0.5m","QSFP-DD","DAC","Coax","Electrical","-","400GE","0.5m","-","C-temp","Datahseet"]
[null,"SO-QDD-4C-CU1-4","QSFP-DD Active Electrical Cable (AEC) 400G Ethernet, AWG32, CMIS4, 1m","QSFP-DD","DAC","Coax","Electrical","-","400GE","1m","-","C-temp","Datahseet"]
[null,"SO-QDD-4C-1CU5-4","QSFP-DD Active Electrical Cable (AEC) 400G Ethernet, AWG32, CMIS4, 1.5m","QSFP-DD","DAC","Coax","Electrical","-","400GE","1.5m","-","C-temp","Datahseet"]
[null,"SO-QDD-4C-CU2-4","QSFP-DD Active Electrical Cable (AEC) 400G Ethernet, AWG32, CMIS4, 2m","QSFP-DD","DAC","Coax","Electrical","-","400GE","2m","-","C-temp","Datahseet"]
[null,"SO-QDD-4C-2CU5-4","QSFP-DD Active Electrical Cable (AEC) 400G Ethernet, AWG32, CMIS4, 2.5m","QSFP-DD","DAC","Coax","Electrical","-","400GE","2.5m","-","C-temp","Datahseet"]
[null,"SO-QDD-4C-CU3-4","QSFP-DD Active Electrical Cable (AEC) 400G Ethernet, AWG32, CMIS4, 3m","QSFP-DD","DAC","Coax","Electrical","-","400GE","3m","-","C-temp","Datahseet"]
[null,"SO-QDD-4C-CU5-4","QSFP-DD Active Electrical Cable (AEC) 400G Ethernet, AWG30, CMIS4, 5m","QSFP-DD","DAC","Coax","Electrical","-","400GE","5m","-","C-temp","Datahseet"]
[null,"SO-QSFPDD-AOC01M","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS3.0 1m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","1m","CMIS3.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC03M","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS3.0 3m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","3m","CMIS3.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC05M","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS3.0 5m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","5m","CMIS3.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC07M","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS3.0 7m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","7m","CMIS3.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC10M","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS3.0 10m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","10m","CMIS3.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC15M","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS3.0 15m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","15m","CMIS3.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC20M","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS3.0 20m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","20m","CMIS3.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC30M","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS3.0 30m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","30m","CMIS3.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC01M-4","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS4.0 1m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","1m","CMIS4.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC03M-4","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS4.0 3m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","3m","CMIS4.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC05M-4","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS4.0 5m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","5m","CMIS4.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC07M-4","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS4.0 7m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","7m","CMIS4.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC10M-4","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS4.0 10m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","10m","CMIS4.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC15M-4","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS4.0 15m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","15m","CMIS4.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC20M-4","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS4.0 20m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","20m","CMIS4.0","C-temp","Datasheet"]
[null,"SO-QSFPDD-AOC30M-4","QSFP-DD 400G Ethernet-SR8, Active Optical Cable AOC MM CMIS4.0 30m","QSFP-DD","AOC","Ribbon","MM","850nm","400GE","30m","CMIS4.0","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC1M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 1m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","1m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC2M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 2m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","2m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC3M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 3m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","3m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC4M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 4m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","4m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC5M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 5m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","5m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC6M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 6m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","6m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC7M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 7m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","7m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC8M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 8m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","8m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC9M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 9m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","9m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC10M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 10m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","10m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC12M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 12m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","12m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC15M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 15m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","15m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC20M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 20m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","20m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC30M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 30m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","30m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-AOC50M","QSFP28 to QSFP28 Active Optical Cable (AOC), 100G Ethernet, 50m ","QSFP28","AOC","Ribbon","MM","850nm","100GE","50m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-CWDM4","QSFP28, 100G Ethernet CWDM4, SM  1271/1291/1311/1331nm, 2km, 5dB, LC","QSFP28","Grey","Fiber-pair","SM","1271/1291/1311/1331nm","100GE","2km","100G-CWDM4","C-temp","Datasheet"]
[null,"SO-QSFP28-ER4","QSFP28, 100G Ethernet ER4, SM  1296/1300/1305/1309nm, 40km, 18dB, LC","QSFP28","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE","40km","100G 4WDM-40","C-temp","Datasheet"]
[null,"TQ2009-SL4E-SO","QSFP28, 100G Ethernet 100G 4WDM-40, SM  1296/1300/1305/1309nm, 40km, 18dB, E-temp, LC","QSFP29","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE","40km","100G 4WDM-40","E-temp","Datasheet"]
[null,"TQ2009-SL4I-SO","QSFP28, 100G Ethernet 100G 4WDM-40, SM  1296/1300/1305/1309nm, 40km, 18dB, I-temp, LC","QSFP28","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE","40km","100G 4WDM-40","I-temp","Datasheet"]
[null,"SO-QSFP28-LR4","QSFP28, 100G Ethernet LR4, OTU4, SM 1296/1300/1305/1309nm, 10km, 6.3dB, LC","QSFP28","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE/OTU4","10km","100GBASE‐LR4","C-temp","Datasheet"]
[null,"SO-QSFP28-LR4-10L","QSFP28, 100G Ethernet LR4, SM  1296/1300/1305/1309nm, 10km, 6.3dB, LC","QSFP28","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE","10km","100GBASE-LR4","C-temp","Datasheet"]
[null,"SO-QSFP28-LR4-20L","QSFP28, 100G Ethernet eLR4, SM, 1296/1300/1305/1309nm, 20km, 8.1dB, LC","QSFP28","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE","20km","100GBASE-LR4","C-temp","Datasheet"]
[null,"SO-QSFP28-PCU0.5M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 0.5m, passive","QSFP28","DAC","Coax","Electrical","-","100GE","0.5m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-PCU1M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 1m, passive","QSFP28","DAC","Coax","Electrical","-","100GE","1m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-PCU2M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 2m, passive","QSFP28","DAC","Coax","Electrical","-","100GE","2m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-PCU3M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 3m, passive","QSFP28","DAC","Coax","Electrical","-","100GE","3m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-PCU5M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG26, 5m, passive","QSFP28","DAC","Coax","Electrical","-","100GE","5m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-LR4-20D","QSFP28, 100G Ethernet eLR4, OTU4 4I1 9D1F, SM, 1296/1300/1305/1309nm, 20km, 12dB, LC","QSFP28","Grey","Fiber-pair","SM","1296/1300/1305/1309nm","100GE/OTU4","20km","100G 4WDM-20","C-temp","Datasheet"]
[null,"SO-QSFP28-PSM4","QSFP28, 100G Ethernet PSM4, SM 4x 1310nm, 2km, 4.7dB, MPO","QSFP28","Grey","Ribbon","SM","4x 1310nm","100GE","2km","100GBASE‐PSM4","C-temp","Datasheet"]
[null,"SO-QSFP28-SR4","QSFP28, 100G Ethernet SR4, MM 4x 850nm, 100m, 1.9dB, MPO","QSFP28","Grey","Ribbon","MM","4x 850nm","100GE","100m","100GBASE-SR4","C-temp","Datasheet"]
[null,"SO-QSFP28-SWDM4","QSFP28, 100G Ethernet SWDM4, MM,  850/880/910/940nm, 150m, 1.8dB, LC","QSFP28","Grey","Fiber-pair","MM","850/880/910/940nm","100GE","150m","100G SWDM4","C-temp","Datasheet"]
[null,"SO-QSFP28-4SFP28-PCU1M","QSFP28 to 4xSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 1m, passive","QSFP28/SFP28","DAC","Coax","Electrical","-","100GE","1m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-4SFP28-PCU2M","QSFP28 to 4xSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 2m, passive","QSFP28/SFP28","DAC","Coax","Electrical","-","100GE","2m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-4SFP28-PCU3M","QSFP28 to 4xSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 3m, passive","QSFP28/SFP28","DAC","Coax","Electrical","-","100GE","3m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-4SFP28-PCU5M","QSFP28 to 4xSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG26, 5m, passive","QSFP28/SFP28","DAC","Coax","Electrical","-","100GE","5m","-","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC1M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 1m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","1m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC2M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 2m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","2m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC3M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 3m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","3m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC4M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 4m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","4m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC5M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 5m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","5m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC6M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 6m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","6m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC7M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 7m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","7m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC8M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 8m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","8m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC9M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 9m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","9m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC10M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 10m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","10m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC12M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 12m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","12m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC15M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 15m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","15m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC20M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 20m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","20m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC30M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 30m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","30m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC50M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 50m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","50m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-QSFP28-4XSFP28-AOC70M","QSFP28 to 4xSFP28, Active Optical Cable (AOC), 100G to 4x 25G Eth, 70m","QSFP28/SFP28","AOC","Fiber-pair","MM","850nm","100GE/25GE","70m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX10D-34","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1310/1490nm, SM, 10km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","1GbE/FE/1G FC","10km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX10D-34-I","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1310/1490nm, SM, 10km, 13dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","1GbE/FE/1G FC","10km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX10D-35","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, SM, 10km, 12dB, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","1GbE/1G FC","10km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX10D-35-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, SM, 10km, 12dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","1GbE/1G FC","10km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX10D-43","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1310nm, SM, 10km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC","10km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX10D-43-I","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1310nm, SM, 10km, 13dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC","10km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX10D-53","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, SM, 10km, 12dB, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/1G FC","10km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX10D-53-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, SM, 10km, 12dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/1G FC","10km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX160D-5157","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1510/1570nm, SM, 160km, 34dB, LC","SFP","BiDi","Single-fiber","SM","1510/1570nm","1GbE/FE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX160D-5157-E","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1510/1570nm, SM, 160km, 34dB, E-temp, LC","SFP","BiDi","Single-fiber","SM","1510/1570nm","1GbE/FE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX160D-5751","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1570/1510nm, SM, 160km, 34dB, LC","SFP","BiDi","Single-fiber","SM","1570/1510nm","1GbE/FE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX160D-5751-E","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1570/1510nm, SM, 160km, 34dB, E-temp, LC","SFP","BiDi","Single-fiber","SM","1570/1510nm","1GbE/FE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX80D-4955","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1550nm, SM, 80km, 26dB, LC","SFP","BiDi","Single-fiber","SM","1490/1550nm","1GbE/FE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX80D-4955-E","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1550nm, SM, 80km, 26dB, E-temp, LC","SFP","BiDi","Single-fiber","SM","1490/1550nm","1GbE/FE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX80D-5549","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1550/1490nm, SM, 80km, 26dB, LC","SFP","BiDi","Single-fiber","SM","1550/1490nm","1GbE/FE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX80D-5549-E","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1550/1490nm, SM, 80km, 26dB, E-temp, LC","SFP","BiDi","Single-fiber","SM","1550/1490nm","1GbE/FE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX20D-34","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1310/1490nm, SM, 20km, 14dB, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","1GbE/FE/1G FC","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX20D-34-I","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1310/1490nm, SM, 20km, 14dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","1GbE/FE/1G FC","20km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX20D-35","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, SM, 20km, 14dB, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","1GbE/1G FC","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX20D-35-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, SM, 20km, 14dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","1GbE/1G FC","20km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX20D-43","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1310nm, SM, 20km, 14dB, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX20D-43-I","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1310nm, SM, 20km, 14dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC","20km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX20D-53","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, SM, 20km, 14dB, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/1G FC","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX20D-53-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, SM, 20km, 14dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/1G FC","20km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX40D-34","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1310/1490nm, SM, 40km, 19dB, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","1GbE/FE/1G FC","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX40D-34-I","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1310/1490nm, SM, 40km, 19dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","1GbE/FE/1G FC","40km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX40D-35","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, SM, 40km, 20dB, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","1GbE/1G FC","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX40D-35-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, SM, 40km, 20dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","1GbE/1G FC","40km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX40D-43","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1310nm, SM, 40km, 19dB, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX40D-43-I","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1310nm, SM, 40km, 19dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC","40km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX40D-53","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, SM, 40km, 18dB, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/1G FC","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX40D-53-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, SM, 40km, 18dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/1G FC","40km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX60D-34","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1310/1490nm, SM, 60km, 27dB, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","1GbE/FE/1G FC","60km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX60D-34-I","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1310/1490nm, SM, 60km, 27dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","1GbE/FE/1G FC","60km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX60D-35","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, SM, 60km, 20dB, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","1GbE/1G FC","60km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX60D-35-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, SM, 60km, 20dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","1GbE/1G FC","60km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX60D-43","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1310nm, SM, 60km, 27dB, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC","60km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX60D-43-I","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1490/1310nm, SM, 60km, 27dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","1GbE/FE/1G FC","60km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX60D-53","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, SM, 60km, 19dB, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/1G FC","60km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX60D-53-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, SM, 60km, 19dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","1GbE/1G FC","60km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX80D-5157","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1510/1570nm, SM, 80km, 26dB, LC","SFP","BiDi","Single-fiber","SM","1510/1570nm","1GbE/FE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX80D-5157-E","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1510/1570nm, SM, 80km, 26dB, E-temp, LC","SFP","BiDi","Single-fiber","SM","1510/1570nm","1GbE/FE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX80D-5751","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1570/1510nm, SM, 80km, 26dB, LC","SFP","BiDi","Single-fiber","SM","1570/1510nm","1GbE/FE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX80D-5751-E","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1570/1510nm, SM, 80km, 26dB, E-temp, LC","SFP","BiDi","Single-fiber","SM","1570/1510nm","1GbE/FE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX-MMD-35","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, MM, 1km, 11dB, LC","SFP","BiDi","Single-fiber","MM","1310/1550nm","1GbE/1G FC","1km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX-MMD-35-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1310/1550nm, MM, 1km, 11dB, I-temp, LC","SFP","BiDi","Single-fiber","MM","1310/1550nm","1GbE/1G FC","1km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX-MMD-53","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, MM, 1km, 11dB, LC","SFP","BiDi","Single-fiber","MM","1550/1310nm","1GbE/1G FC","1km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX-MMD-53-I","SFP, BiDi, 1G Ethernet, 1G FC, TX/RX=1550/1310nm, MM, 1km, 11dB, I-temp, LC","SFP","BiDi","Single-fiber","MM","1550/1310nm","1GbE/1G FC","1km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-EZXD","SFP, 1G Ethernet, 1G FC, SM 1550nm, 120km, 32dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-EZXD-I","SFP, 1G Ethernet, 1G FC, SM 1550nm, 120km, 32dB, I-temp, LC","SFP","Grey","Fiber-pair","SM","1550nm","1GbE/1G FC","120km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-L20D","SFP, 1G Ethernet, 1G FC, SM 1310nm, 20km, 14dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","1GbE/1G FC","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-L20D-I","SFP, 1G Ethernet, 1G FC, SM 1310nm, 20km, 14dB, I-temp, LC","SFP","Grey","Fiber-pair","SM","1310nm","1GbE/1G FC","20km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-L40D","SFP, 1G Ethernet, 1G FC, SM 1310nm, 40km, 22dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","1GbE/1G FC","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-L40D-I","SFP, 1G Ethernet, 1G FC, SM 1310nm, 40km, 22dB, I-temp, LC","SFP","Grey","Fiber-pair","SM","1310nm","1GbE/1G FC","40km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-LXD","SFP, 1G Ethernet, 1G FC, SM 1310nm, 10km, 12dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","1GbE/1G FC","10km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-LXD-I","SFP, 1G Ethernet, 1G FC, SM 1310nm, 10km, 12dB, I-temp, LC","SFP","Grey","Fiber-pair","SM","1310nm","1GbE/1G FC","10km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-MMXD","SFP, Multirate 125Mbps-1.25Gbps, MM 1310nm, 1km@OM3, 12dB, LC","SFP","Grey","Fiber-pair","MM","1310nm","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","1km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-MMXD-I","SFP, Multirate 125Mbps-1.25Gbps, MM 1310nm, 1km@OM3, 12dB, I-temp, LC","SFP","Grey","Fiber-pair","MM","1310nm","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","1km","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-SXD","SFP, 1G Ethernet, 1G FC, MM 850nm, 550m@OM3, 7.5dB, LC","SFP","Grey","Fiber-pair","MM","850nm","1GbE/1G FC","550m","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-SXD-I","SFP, 1G Ethernet, 1G FC, MM 850nm, 550m@OM3, 7.5dB, I-temp, LC","SFP","Grey","Fiber-pair","MM","850nm","1GbE/1G FC","550m","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-T","SFP, 1G Ethernet, 100m@CAT5, RJ45","SFP","Grey","LAN","Electrical","-","1GbE","100m","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-T-I","SFP, 1G Ethernet, 100m@CAT5, I-temp, RJ45","SFP","Grey","LAN","Electrical","-","1GbE","100m","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-TR","SFP, 1G Ethernet, 100m@CAT5, RJ45","SFP","Grey","LAN","Electrical","-","1GbE","100m","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-TR-I","SFP, 1G Ethernet, 100m@CAT5, I-temp, RJ45","SFP","Grey","LAN","Electrical","-","1GbE","100m","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-TX","SFP, 1G/100M/10M Ethernet, SERDES/SGMII Interface, 100m, RJ45","SFP","Grey","LAN","Electrical","-","1GbE/FE/10M","100m","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-TX-I","SFP, 1G/100M/10M Ethernet, SERDES/SGMII Interface, 100m, I-temp, RJ45","SFP","Grey","LAN","Electrical","-","1GbE/FE/10M","100m","-","I-temp","Datasheet"]
[null,"SO-SFP-1000Base-ZXD","SFP, 1G Ethernet, 1G FC, SM 1550nm, 80km, 24dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-ZXD-I","SFP, 1G Ethernet, 1G FC, SM 1550nm, 80km, 24dB, I-temp, LC","SFP","Grey","Fiber-pair","SM","1550nm","1GbE/1G FC","80km","-","I-temp","Datasheet"]
[null,"SO-SFP-100Base-BX20D-34","SFP, BiDi, 100M Ethernet, STM-1/OC3, TX/RX=1310/1490nm, SM, 20km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","STM-1/OC-3/FE","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-BX20D-35","SFP, BiDi, 100M Ethernet, STM-1/OC3, TX/RX=1310/1550nm, SM, 20km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","STM-1/OC-3/FE","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-BX20D-43","SFP, BiDi, 100M Ethernet, STM-1/OC3, TX/RX=1490/1310nm, SM, 20km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","STM-1/OC-3/FE","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-BX20D-53","SFP, BiDi, 100M Ethernet, STM-1/OC3, TX/RX=1550/1310nm, SM, 20km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","STM-1/OC-3/FE","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-BX40D-35","SFP, BiDi, 100M Ethernet, STM-1/OC3, TX/RX=1310/1550nm, SM, 40km, 28dB, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-BX40D-53","SFP, BiDi, 100M Ethernet, STM-1/OC3, TX/RX=1550/1310nm, SM, 40km, 28dB, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-EXD","SFP, 100M Ethernet, STM-1/OC3, SM 1310nm, 40km, 29dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-FXD-I","SFP, 100M Ethernet, STM-1/OC3, MM 1310nm, 2km, 12dB, LC, I-temp","SFP","Grey","Fiber-pair","MM","1310nm","STM-1/OC-3/FE","2km","-","I-temp","Datasheet"]
[null,"SO-SFP-100Base-FXD","SFP, 100M Ethernet, STM-1/OC3, MM 1310nm, 2km, 12dB, LC","SFP","Grey","Fiber-pair","MM","1310nm","STM-1/OC-3/FE","2km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L160D","SFP, 100M Ethernet, STM-1/OC3, SM 1550nm, 160km, 37dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L160D-C47","SFP, 100M Ethernet, STM-1/OC3, CWDM, 160km, 37dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L160D-C49","SFP, 100M Ethernet, STM-1/OC3, CWDM, 160km, 37dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L160D-C51","SFP, 100M Ethernet, STM-1/OC3, CWDM, 160km, 37dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L160D-C53","SFP, 100M Ethernet, STM-1/OC3, CWDM, 160km, 37dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L160D-C55","SFP, 100M Ethernet, STM-1/OC3, CWDM, 160km, 37dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L160D-C57","SFP, 100M Ethernet, STM-1/OC3, CWDM, 160km, 37dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L160D-C59","SFP, 100M Ethernet, STM-1/OC3, CWDM, 160km, 37dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L160D-C61","SFP, 100M Ethernet, STM-1/OC3, CWDM, 160km, 37dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L200D","SFP, 100M Ethernet, STM-1/OC3, SM 1550nm, 200km, 47dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L200D-C47","SFP, 100M Ethernet, STM-1/OC3, CWDM, 200km, 47dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L200D-C49","SFP, 100M Ethernet, STM-1/OC3, CWDM, 200km, 47dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L200D-C51","SFP, 100M Ethernet, STM-1/OC3, CWDM, 200km, 47dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L200D-C53","SFP, 100M Ethernet, STM-1/OC3, CWDM, 200km, 47dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L200D-C55","SFP, 100M Ethernet, STM-1/OC3, CWDM, 200km, 47dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L200D-C57","SFP, 100M Ethernet, STM-1/OC3, CWDM, 200km, 47dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L200D-C59","SFP, 100M Ethernet, STM-1/OC3, CWDM, 200km, 47dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L200D-C61","SFP, 100M Ethernet, STM-1/OC3, CWDM, 200km, 47dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L80D-C47","SFP, 100M Ethernet, STM-1/OC3, CWDM, 80km, 29dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L80D-C49","SFP, 100M Ethernet, STM-1/OC3, CWDM, 80km, 29dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L80D-C51","SFP, 100M Ethernet, STM-1/OC3, CWDM, 80km, 29dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L80D-C53","SFP, 100M Ethernet, STM-1/OC3, CWDM, 80km, 29dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L80D-C55","SFP, 100M Ethernet, STM-1/OC3, CWDM, 80km, 29dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L80D-C57","SFP, 100M Ethernet, STM-1/OC3, CWDM, 80km, 29dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L80D-C59","SFP, 100M Ethernet, STM-1/OC3, CWDM, 80km, 29dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-L80D-C61","SFP, 100M Ethernet, STM-1/OC3, CWDM, 80km, 29dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-LXD","SFP, 100M Ethernet, STM-1/OC3, SM 1310nm, 15km, 13dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","STM-1/OC-3/FE","15km","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-T-I","SFP, 100M/10M Ethernet, 100m@CAT5, RJ45, I-temp","SFP","Grey","LAN","Electrical",null,"FE/10M","100m","-","I-temp","Datasheet"]
[null,"SO-SFP-100Base-T","SFP, 100M/10M Ethernet, 100m@CAT5, RJ45","SFP","Grey","LAN","Electrical","-","FE/10M","100m","-","C-temp","Datasheet"]
[null,"SO-SFP-100Base-ZXD","SFP, 100M Ethernet, STM-1/OC3, SM 1550nm, 80km, 29dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L15D","SFP, STM-1/OC3, 100M Ethernet, SM 1310nm, 15km, 13dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","STM-1/OC-3/FE","15km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D","SFP, STM-1/OC3, 100M Ethernet, SM 1550nm, 160km, 37dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C27","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C29","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C31","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C33","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C35","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C37","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C39","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C41","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C43","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C45","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C47","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C49","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C51","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C53","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C55","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C57","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C59","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L160D-C61","SFP, STM-1/OC3, 100M Ethernet, CWDM, 160km, 37dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L200D","SFP, STM-1/OC3, 100M Ethernet, SM 1550nm, 200km, 47dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","200km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L260D-C47","SFP, STM-1/OC3, 100M Ethernet, CWDM, 260km, 46dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-1/OC-3/FE","260km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L260D-C49","SFP, STM-1/OC3, 100M Ethernet, CWDM, 260km, 46dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-1/OC-3/FE","260km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L260D-C51","SFP, STM-1/OC3, 100M Ethernet, CWDM, 260km, 46dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-1/OC-3/FE","260km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L260D-C53","SFP, STM-1/OC3, 100M Ethernet, CWDM, 260km, 46dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-1/OC-3/FE","260km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L260D-C55","SFP, STM-1/OC3, 100M Ethernet, CWDM, 260km, 46dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","260km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L260D-C57","SFP, STM-1/OC3, 100M Ethernet, CWDM, 260km, 46dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-1/OC-3/FE","260km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L260D-C59","SFP, STM-1/OC3, 100M Ethernet, CWDM, 260km, 46dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-1/OC-3/FE","260km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L260D-C61","SFP, STM-1/OC3, 100M Ethernet, CWDM, 260km, 46dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-1/OC-3/FE","260km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L270D-C47","SFP, STM-1/OC3, 100M Ethernet, CWDM, 270km, 50dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-1/OC-3/FE","270km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L270D-C49","SFP, STM-1/OC3, 100M Ethernet, CWDM, 270km, 50dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-1/OC-3/FE","270km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L270D-C51","SFP, STM-1/OC3, 100M Ethernet, CWDM, 270km, 50dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-1/OC-3/FE","270km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L270D-C53","SFP, STM-1/OC3, 100M Ethernet, CWDM, 270km, 50dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-1/OC-3/FE","270km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L270D-C55","SFP, STM-1/OC3, 100M Ethernet, CWDM, 270km, 50dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","270km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L270D-C57","SFP, STM-1/OC3, 100M Ethernet, CWDM, 270km, 50dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-1/OC-3/FE","270km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L270D-C59","SFP, STM-1/OC3, 100M Ethernet, CWDM, 270km, 50dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-1/OC-3/FE","270km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L270D-C61","SFP, STM-1/OC3, 100M Ethernet, CWDM, 270km, 50dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-1/OC-3/FE","270km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-O-C49-E","SFP FE/155M 34dB, OTDR 65dB, E-temp, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-1/OC-3/FE","100km","-","E-temp","Datasheet"]
[null,"SO-SFP-155M-O-C51-E","SFP FE/155M 34dB, OTDR 65dB, E-temp, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-1/OC-3/FE","100km","-","E-temp","Datasheet"]
[null,"SO-SFP-1G-O-C49-E","SFP FE/1G 23dB, OTDR 65dB, E-temp, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/FE","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-1G-O-C51-E","SFP FE/1G 23dB, OTDR 65dB, E-temp, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/FE","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-155M-L2D","SFP, STM-1/OC3, 100M Ethernet, MM 1310nm, 2km, 12dB, LC","SFP","Grey","Fiber-pair","MM","1310nm","STM-1/OC-3/FE","2km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L40D","SFP, STM-1/OC3, 100M Ethernet, SM 1310nm, 40km, 29dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D","SFP, STM-1/OC3, 100M Ethernet, SM 1550nm, 80km, 29dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C27","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C29","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C31","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C33","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C35","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C37","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C39","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C41","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C43","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C45","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C47","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C49","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C51","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C53","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C55","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C57","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C59","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L80D-C61","SFP, STM-1/OC3, 100M Ethernet, CWDM, 80km, 29dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, SM 1550nm, 120km, 34dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-155M-L120D-C51","SFP, STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D-C31","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D-C47","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D-C49","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D-C51","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D-C53","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D-C55","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D-C57","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D-C59","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L120D-C61","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 120km, 34dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-4/OC-12/STM-1/OC-3/FE","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L15D","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, SM 1310nm, 15km, 13dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","STM-4/OC-12/STM-1/OC-3/FE","2km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L160D","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, SM 1550nm, 160km, 38dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM-4/OC-12/STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L160D-C47","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, CWDM, 160km, 41dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-4/OC-12/STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L160D-C49","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, CWDM, 160km, 41dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-4/OC-12/STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L160D-C51","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, CWDM, 160km, 41dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-4/OC-12/STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L160D-C53","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, CWDM, 160km, 41dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-4/OC-12/STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L160D-C55","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, CWDM, 160km, 41dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-4/OC-12/STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L160D-C57","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, CWDM, 160km, 41dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-4/OC-12/STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L160D-C59","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, CWDM, 160km, 41dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-4/OC-12/STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L160D-C61","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, CWDM, 160km, 41dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-4/OC-12/STM-1/OC-3/FE","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L2D","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, MM 1310nm, 2km, 8dB, LC","SFP","Grey","Fiber-pair","MM","1310nm","STM-4/OC-12/STM-1/OC-3/FE","2km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L40D","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, SM 1310nm, 40km, 25dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","STM-4/OC-12/STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L40D-C47","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 40km, 23dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-4/OC-12/STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L40D-C49","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 40km, 23dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-4/OC-12/STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L40D-C51","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 40km, 23dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-4/OC-12/STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L40D-C53","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 40km, 23dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-4/OC-12/STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L40D-C55","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 40km, 23dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-4/OC-12/STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L40D-C57","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 40km, 23dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-4/OC-12/STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L40D-C59","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 40km, 23dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-4/OC-12/STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L40D-C61","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 40km, 23dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-4/OC-12/STM-1/OC-3/FE","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L80D","SFP, STM-4/OC12, STM-1/OC3, 100M Ethernet, SM 1550nm, 80km, 25dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM-4/OC-12/STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L80D-C47","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 80km, 28dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM-4/OC-12/STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L80D-C49","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 80km, 28dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM-4/OC-12/STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L80D-C51","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 80km, 28dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM-4/OC-12/STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L80D-C53","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 80km, 28dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM-4/OC-12/STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L80D-C55","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 80km, 28dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM-4/OC-12/STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L80D-C57","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 80km, 28dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM-4/OC-12/STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L80D-C59","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 80km, 28dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM-4/OC-12/STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-622M-L80D-C61","SFP, STM-4/OC12,STM-1/OC3, 100M Ethernet, CWDM, 80km, 28dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM-4/OC-12/STM-1/OC-3/FE","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-GE-FE-BX20D-35","SFP, BiDi, 100M Ethernet, SGMII, TX/RX=1310/1550nm, SM, 20km, 17dB, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","FE","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-GE-FE-BX20D-53","SFP, BiDi, 100M Ethernet, SGMII, TX/RX=1550/1310nm, SM, 20km, 17dB, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","FE","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-GE-FE-FX","SFP, 100M Ethernet FX, SGMII, MM 1310nm, 2km, 10dB, LC","SFP","Grey","Fiber-pair","MM","1310nm","FE/SGMII","2km","-","C-temp","Datasheet"]
[null,"SO-SFP-GE-FE-LX","SFP, 100M Ethernet LX, SGMII, SM 1310nm, 10km, 16dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","FE/SGMII","10km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C27","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C29","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C31","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C33","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C35","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C37","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C39","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C41","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C43","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C45","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C47","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C49","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C51","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C53","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C55","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C57","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C59","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C61","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-C27-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1270nm  ","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C29-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1290nm  ","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C31-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1310nm  ","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C33-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1330nm  ","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C35-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1350nm  ","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C37-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1370nm  ","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C39-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1390nm  ","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C41-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1410nm  ","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C43-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1430nm  ","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C45-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1450nm  ","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C47-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1470nm  ","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C49-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1490nm  ","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C51-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1510nm  ","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C53-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1530nm  ","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C55-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1550nm  ","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C57-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1570nm  ","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C59-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1590nm  ","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-C61-E","SFP, 1G Ethernet, 1G FC, CWDM, 120km, 34dB, E-temp, LC, 1610nm  ","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D919","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D919","SFP","DWDM/100GHz","Fiber-pair","SM"," D9190","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D920","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D920","SFP","DWDM/100GHz","Fiber-pair","SM"," D9200","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D921","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D921","SFP","DWDM/100GHz","Fiber-pair","SM"," D9210","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D922","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D922","SFP","DWDM/100GHz","Fiber-pair","SM"," D9220","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D923","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D923","SFP","DWDM/100GHz","Fiber-pair","SM"," D9230","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D924","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D924","SFP","DWDM/100GHz","Fiber-pair","SM"," D9240","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D925","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D925","SFP","DWDM/100GHz","Fiber-pair","SM"," D9250","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D926","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D926","SFP","DWDM/100GHz","Fiber-pair","SM"," D9260","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D927","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D927","SFP","DWDM/100GHz","Fiber-pair","SM"," D9270","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D928","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D928","SFP","DWDM/100GHz","Fiber-pair","SM"," D9280","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D929","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D929","SFP","DWDM/100GHz","Fiber-pair","SM"," D9290","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D930","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D930","SFP","DWDM/100GHz","Fiber-pair","SM"," D9300","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D931","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D931","SFP","DWDM/100GHz","Fiber-pair","SM"," D9310","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D932","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D932","SFP","DWDM/100GHz","Fiber-pair","SM"," D9320","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D933","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D933","SFP","DWDM/100GHz","Fiber-pair","SM"," D9330","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D934","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D934","SFP","DWDM/100GHz","Fiber-pair","SM"," D9340","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D935","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D935","SFP","DWDM/100GHz","Fiber-pair","SM"," D9350","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D936","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D936","SFP","DWDM/100GHz","Fiber-pair","SM"," D9360","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D937","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D937","SFP","DWDM/100GHz","Fiber-pair","SM"," D9370","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D938","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D938","SFP","DWDM/100GHz","Fiber-pair","SM"," D9380","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D939","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D939","SFP","DWDM/100GHz","Fiber-pair","SM"," D9390","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D940","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D940","SFP","DWDM/100GHz","Fiber-pair","SM"," D9400","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D941","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D941","SFP","DWDM/100GHz","Fiber-pair","SM"," D9410","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D942","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D942","SFP","DWDM/100GHz","Fiber-pair","SM"," D9420","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D943","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D943","SFP","DWDM/100GHz","Fiber-pair","SM"," D9430","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D944","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D944","SFP","DWDM/100GHz","Fiber-pair","SM"," D9440","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D945","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D945","SFP","DWDM/100GHz","Fiber-pair","SM"," D9450","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D946","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D946","SFP","DWDM/100GHz","Fiber-pair","SM"," D9460","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D947","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D947","SFP","DWDM/100GHz","Fiber-pair","SM"," D9470","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D948","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D948","SFP","DWDM/100GHz","Fiber-pair","SM"," D9480","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D949","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D949","SFP","DWDM/100GHz","Fiber-pair","SM"," D9490","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D950","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D950","SFP","DWDM/100GHz","Fiber-pair","SM"," D9500","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D951","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D951","SFP","DWDM/100GHz","Fiber-pair","SM"," D9510","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D952","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D952","SFP","DWDM/100GHz","Fiber-pair","SM"," D9520","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D953","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D953","SFP","DWDM/100GHz","Fiber-pair","SM"," D9530","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D954","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D954","SFP","DWDM/100GHz","Fiber-pair","SM"," D9540","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D955","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D955","SFP","DWDM/100GHz","Fiber-pair","SM"," D9550","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D956","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D956","SFP","DWDM/100GHz","Fiber-pair","SM"," D9560","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D957","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D957","SFP","DWDM/100GHz","Fiber-pair","SM"," D9570","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D958","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D958","SFP","DWDM/100GHz","Fiber-pair","SM"," D9580","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D959","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D959","SFP","DWDM/100GHz","Fiber-pair","SM"," D9590","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D960","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, LC, D960","SFP","DWDM/100GHz","Fiber-pair","SM"," D9600","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120D-D919-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D919 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9190","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D920-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D920 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9200","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D921-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D921 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9210","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D922-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D922 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9220","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D923-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D923 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9230","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D924-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D924 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9240","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D925-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D925 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9250","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D926-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D926 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9260","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D927-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D927 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9270","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D928-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D928 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9280","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D929-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D929 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9290","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D930-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D930 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9300","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D931-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D931 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9310","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D932-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D932 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9320","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D933-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D933 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9330","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D934-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D934 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9340","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D935-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D935 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9350","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D936-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D936 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9360","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D937-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D937 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9370","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D938-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D938 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9380","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D939-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D939 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9390","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D940-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D940 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9400","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D941-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D941 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9410","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D942-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D942 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9420","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D943-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D943 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9430","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D944-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D944 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9440","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D945-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D945 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9450","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D946-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D946 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9460","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D947-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D947 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9470","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D948-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D948 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9480","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D949-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D949 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9490","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D950-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D950 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9500","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D951-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D951 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9510","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D952-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D952 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9520","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D953-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D953 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9530","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D954-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D954 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9540","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D955-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D955 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9550","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D956-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D956 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9560","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D957-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D957 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9570","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D958-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D958 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9580","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D959-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D959 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9590","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120D-D960-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 120km, 32dB, E-temp, LC, D960 ","SFP","DWDM/100GHz","Fiber-pair","SM"," D9600","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-L120DH-D919","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D919","SFP","DWDM/100GHz","Fiber-pair","SM"," D9190","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D920","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D920","SFP","DWDM/100GHz","Fiber-pair","SM"," D9200","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D921","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D921","SFP","DWDM/100GHz","Fiber-pair","SM"," D9210","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D922","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D922","SFP","DWDM/100GHz","Fiber-pair","SM"," D9220","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D923","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D923","SFP","DWDM/100GHz","Fiber-pair","SM"," D9230","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D924","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D924","SFP","DWDM/100GHz","Fiber-pair","SM"," D9240","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D925","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D925","SFP","DWDM/100GHz","Fiber-pair","SM"," D9250","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D926","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D926","SFP","DWDM/100GHz","Fiber-pair","SM"," D9260","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D927","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D927","SFP","DWDM/100GHz","Fiber-pair","SM"," D9270","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D928","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D928","SFP","DWDM/100GHz","Fiber-pair","SM"," D9280","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D929","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D929","SFP","DWDM/100GHz","Fiber-pair","SM"," D9290","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D930","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D930","SFP","DWDM/100GHz","Fiber-pair","SM"," D9300","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D931","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D931","SFP","DWDM/100GHz","Fiber-pair","SM"," D9310","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D932","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D932","SFP","DWDM/100GHz","Fiber-pair","SM"," D9320","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D933","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D933","SFP","DWDM/100GHz","Fiber-pair","SM"," D9330","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D934","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D934","SFP","DWDM/100GHz","Fiber-pair","SM"," D9340","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D935","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D935","SFP","DWDM/100GHz","Fiber-pair","SM"," D9350","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D936","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D936","SFP","DWDM/100GHz","Fiber-pair","SM"," D9360","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D937","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D937","SFP","DWDM/100GHz","Fiber-pair","SM"," D9370","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D938","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D938","SFP","DWDM/100GHz","Fiber-pair","SM"," D9380","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D939","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D939","SFP","DWDM/100GHz","Fiber-pair","SM"," D9390","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D940","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D940","SFP","DWDM/100GHz","Fiber-pair","SM"," D9400","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D941","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D941","SFP","DWDM/100GHz","Fiber-pair","SM"," D9410","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D942","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D942","SFP","DWDM/100GHz","Fiber-pair","SM"," D9420","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D943","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D943","SFP","DWDM/100GHz","Fiber-pair","SM"," D9430","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D944","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D944","SFP","DWDM/100GHz","Fiber-pair","SM"," D9440","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D945","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D945","SFP","DWDM/100GHz","Fiber-pair","SM"," D9450","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D946","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D946","SFP","DWDM/100GHz","Fiber-pair","SM"," D9460","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D947","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D947","SFP","DWDM/100GHz","Fiber-pair","SM"," D9470","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D948","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D948","SFP","DWDM/100GHz","Fiber-pair","SM"," D9480","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D949","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D949","SFP","DWDM/100GHz","Fiber-pair","SM"," D9490","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D950","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D950","SFP","DWDM/100GHz","Fiber-pair","SM"," D9500","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D951","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D951","SFP","DWDM/100GHz","Fiber-pair","SM"," D9510","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D952","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D952","SFP","DWDM/100GHz","Fiber-pair","SM"," D9520","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D953","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D953","SFP","DWDM/100GHz","Fiber-pair","SM"," D9530","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D954","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D954","SFP","DWDM/100GHz","Fiber-pair","SM"," D9540","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D955","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D955","SFP","DWDM/100GHz","Fiber-pair","SM"," D9550","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D956","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D956","SFP","DWDM/100GHz","Fiber-pair","SM"," D9560","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D957","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D957","SFP","DWDM/100GHz","Fiber-pair","SM"," D9570","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D958","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D958","SFP","DWDM/100GHz","Fiber-pair","SM"," D9580","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D959","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D959","SFP","DWDM/100GHz","Fiber-pair","SM"," D9590","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L120DH-D960","SFP Multirate 0.1-1.25Gbps DWDM 100GHz 120km 41dB HighPower LC D960","SFP","DWDM/100GHz","Fiber-pair","SM"," D9600","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C27","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C29","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C31","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C33","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C35","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C37","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C39","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C41","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C43","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C45","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C47","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C49","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C51","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C53","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C55","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C57","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C59","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C61","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160D-C27-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1270nm  ","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C29-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1290nm  ","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C31-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1310nm  ","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C33-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1330nm  ","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C35-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1350nm  ","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C37-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1370nm  ","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C39-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1390nm  ","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C41-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1410nm  ","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C43-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1430nm  ","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C45-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1450nm  ","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C47-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1470nm  ","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C49-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1490nm  ","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C51-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1510nm  ","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C53-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1530nm  ","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C55-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1550nm  ","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C57-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1570nm  ","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C59-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1590nm  ","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160D-C61-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 38dB, E-temp, LC, 1610nm  ","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C27","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C29","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C31","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C33","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C35","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C37","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C39","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C41","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C43","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C45","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C47","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C49","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C51","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C53","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C55","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C57","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C59","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C61","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","160km","-","C-temp","Datasheet"]
[null,"SO-SFP-L160DH-C27-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1270nm  ","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C29-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1290nm  ","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C31-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1310nm  ","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C33-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1330nm  ","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C35-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1350nm  ","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C37-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1370nm  ","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C39-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1390nm  ","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C41-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1410nm  ","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C43-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1430nm  ","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C45-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1450nm  ","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C47-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1470nm  ","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C49-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1490nm  ","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C51-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1510nm  ","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C53-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1530nm  ","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C55-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1550nm  ","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C57-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1570nm  ","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C59-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1590nm  ","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L160DH-C61-E","SFP, 1G Ethernet, 1G FC, CWDM, 160km, 41dB HighPower, E-temp, LC, 1610nm  ","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","160km","-","E-temp","Datasheet"]
[null,"SO-SFP-L210D-C27","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C29","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C31","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C33","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C35","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C37","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C39","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C41","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C43","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C45","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C47","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C49","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C51","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C53","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C55","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C57","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C59","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L210D-C61","SFP, 1G Ethernet, 1G FC, CWDM, 210km, 41dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","210km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C27","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C29","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C31","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C33","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C35","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C37","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C39","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C41","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C43","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C45","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C47","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C49","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C51","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C53","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C55","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C57","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C59","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C61","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-L50D-C27-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1270nm ","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C29-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1290nm ","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C31-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1310nm ","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C33-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1330nm ","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C35-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1350nm ","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C37-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1370nm ","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C39-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1390nm ","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C41-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1410nm ","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C43-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1430nm ","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C45-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1450nm ","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C47-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1470nm ","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C49-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1490nm ","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C51-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1510nm ","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C53-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1530nm ","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C55-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1550nm ","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C57-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1570nm ","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C59-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1590nm ","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L50D-C61-E","SFP, 1G Ethernet, 1G FC, CWDM, 50km, 19dB, E-temp, LC, 1610nm ","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","50km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9200","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9200","SFP","DWDM/50GHz","Fiber-pair","SM","D9200 ","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9205","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9205","SFP","DWDM/50GHz","Fiber-pair","SM","D9205","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9210","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9210","SFP","DWDM/50GHz","Fiber-pair","SM","D9210","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9215","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9215","SFP","DWDM/50GHz","Fiber-pair","SM","D9215","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9220","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9220","SFP","DWDM/50GHz","Fiber-pair","SM","D9220","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9225","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9225","SFP","DWDM/50GHz","Fiber-pair","SM","D9225","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9230","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9230","SFP","DWDM/50GHz","Fiber-pair","SM","D9230","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9235","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9235","SFP","DWDM/50GHz","Fiber-pair","SM","D9235","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9240","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9240","SFP","DWDM/50GHz","Fiber-pair","SM","D9240","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9245","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9245","SFP","DWDM/50GHz","Fiber-pair","SM","D9245","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9250","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9250","SFP","DWDM/50GHz","Fiber-pair","SM","D9250","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9255","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9255","SFP","DWDM/50GHz","Fiber-pair","SM","D9255","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9260","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9260","SFP","DWDM/50GHz","Fiber-pair","SM","D9260","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9265","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9265","SFP","DWDM/50GHz","Fiber-pair","SM","D9265","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9270","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9270","SFP","DWDM/50GHz","Fiber-pair","SM","D9270","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9275","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9275","SFP","DWDM/50GHz","Fiber-pair","SM","D9275","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9280","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9280","SFP","DWDM/50GHz","Fiber-pair","SM","D9280","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9285","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9285","SFP","DWDM/50GHz","Fiber-pair","SM","D9285","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9290","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9290","SFP","DWDM/50GHz","Fiber-pair","SM","D9290","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9295","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9295","SFP","DWDM/50GHz","Fiber-pair","SM","D9295","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9300","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9300","SFP","DWDM/50GHz","Fiber-pair","SM","D9300","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9305","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9305","SFP","DWDM/50GHz","Fiber-pair","SM","D9305","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9310","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9310","SFP","DWDM/50GHz","Fiber-pair","SM","D9310","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9315","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9315","SFP","DWDM/50GHz","Fiber-pair","SM","D9315","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9320","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9320","SFP","DWDM/50GHz","Fiber-pair","SM","D9320","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9325","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9325","SFP","DWDM/50GHz","Fiber-pair","SM","D9325","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9330","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9330","SFP","DWDM/50GHz","Fiber-pair","SM","D9330","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9335","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9335","SFP","DWDM/50GHz","Fiber-pair","SM","D9335","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9340","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9340","SFP","DWDM/50GHz","Fiber-pair","SM","D9340","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9345","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9345","SFP","DWDM/50GHz","Fiber-pair","SM","D9345","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9350","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9350","SFP","DWDM/50GHz","Fiber-pair","SM","D9350","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9355","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9355","SFP","DWDM/50GHz","Fiber-pair","SM","D9355","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9360","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9360","SFP","DWDM/50GHz","Fiber-pair","SM","D9360","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9365","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9365","SFP","DWDM/50GHz","Fiber-pair","SM","D9365","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9370","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9370","SFP","DWDM/50GHz","Fiber-pair","SM","D9370","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9375","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9375","SFP","DWDM/50GHz","Fiber-pair","SM","D9375","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9380","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9380","SFP","DWDM/50GHz","Fiber-pair","SM","D9380","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9385","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9385","SFP","DWDM/50GHz","Fiber-pair","SM","D9385","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9390","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9390","SFP","DWDM/50GHz","Fiber-pair","SM","D9390","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9395","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9395","SFP","DWDM/50GHz","Fiber-pair","SM","D9395","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9400","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9400","SFP","DWDM/50GHz","Fiber-pair","SM","D9400","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9405","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9405","SFP","DWDM/50GHz","Fiber-pair","SM","D9405","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9410","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9410","SFP","DWDM/50GHz","Fiber-pair","SM","D9410","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9415","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9415","SFP","DWDM/50GHz","Fiber-pair","SM","D9415","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9420","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9420","SFP","DWDM/50GHz","Fiber-pair","SM","D9420","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9425","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9425","SFP","DWDM/50GHz","Fiber-pair","SM","D9425","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9430","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9430","SFP","DWDM/50GHz","Fiber-pair","SM","D9430","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9435","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9435","SFP","DWDM/50GHz","Fiber-pair","SM","D9435","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9440","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9440","SFP","DWDM/50GHz","Fiber-pair","SM","D9440","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9445","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9445","SFP","DWDM/50GHz","Fiber-pair","SM","D9445","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9450","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9450","SFP","DWDM/50GHz","Fiber-pair","SM","D9450","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9455","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9455","SFP","DWDM/50GHz","Fiber-pair","SM","D9455","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9460","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9460","SFP","DWDM/50GHz","Fiber-pair","SM","D9460","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9465","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9465","SFP","DWDM/50GHz","Fiber-pair","SM","D9465","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9470","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9470","SFP","DWDM/50GHz","Fiber-pair","SM","D9470","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9475","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9475","SFP","DWDM/50GHz","Fiber-pair","SM","D9475","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9480","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9480","SFP","DWDM/50GHz","Fiber-pair","SM","D9480","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9485","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9485","SFP","DWDM/50GHz","Fiber-pair","SM","D9485","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9490","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9490","SFP","DWDM/50GHz","Fiber-pair","SM","D9490","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9495","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9495","SFP","DWDM/50GHz","Fiber-pair","SM","D9495","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9500","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9500","SFP","DWDM/50GHz","Fiber-pair","SM","D9500","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9505","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9505","SFP","DWDM/50GHz","Fiber-pair","SM","D9505","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9510","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9510","SFP","DWDM/50GHz","Fiber-pair","SM","D9510","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9515","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9515","SFP","DWDM/50GHz","Fiber-pair","SM","D9515","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9520","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9520","SFP","DWDM/50GHz","Fiber-pair","SM","D9520","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9525","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9525","SFP","DWDM/50GHz","Fiber-pair","SM","D9525","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9530","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9530","SFP","DWDM/50GHz","Fiber-pair","SM","D9530","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9535","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9535","SFP","DWDM/50GHz","Fiber-pair","SM","D9535","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9540","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9540","SFP","DWDM/50GHz","Fiber-pair","SM","D9540","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9545","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9545","SFP","DWDM/50GHz","Fiber-pair","SM","D9545","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9550","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9550","SFP","DWDM/50GHz","Fiber-pair","SM","D9550","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9555","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9555","SFP","DWDM/50GHz","Fiber-pair","SM","D9555","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9560","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9560","SFP","DWDM/50GHz","Fiber-pair","SM","D9560","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9565","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9565","SFP","DWDM/50GHz","Fiber-pair","SM","D9565","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9570","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9570","SFP","DWDM/50GHz","Fiber-pair","SM","D9570","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9575","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9575","SFP","DWDM/50GHz","Fiber-pair","SM","D9575","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9580","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9580","SFP","DWDM/50GHz","Fiber-pair","SM","D9580","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9585","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9585","SFP","DWDM/50GHz","Fiber-pair","SM","D9585","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9590","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9590","SFP","DWDM/50GHz","Fiber-pair","SM","D9590","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-50G-D9595","SFP Multirate 0.1-1.25Gbps DWDM 50GHz 80km 28dB LC D9595","SFP","DWDM/50GHz","Fiber-pair","SM","D9595","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C27","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C29","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C31","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C33","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C35","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C37","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C39","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C41","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C43","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C45","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C47","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C49","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C51","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C53","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C55","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C57","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C59","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C61","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-C27-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1270nm ","SFP","CWDM","Fiber-pair","SM","1270nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C29-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1290nm ","SFP","CWDM","Fiber-pair","SM","1290nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C31-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1310nm ","SFP","CWDM","Fiber-pair","SM","1310nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C33-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1330nm ","SFP","CWDM","Fiber-pair","SM","1330nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C35-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1350nm ","SFP","CWDM","Fiber-pair","SM","1350nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C37-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1370nm ","SFP","CWDM","Fiber-pair","SM","1370nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C39-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1390nm ","SFP","CWDM","Fiber-pair","SM","1390nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C41-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1410nm ","SFP","CWDM","Fiber-pair","SM","1410nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C43-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1430nm ","SFP","CWDM","Fiber-pair","SM","1430nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C45-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1450nm ","SFP","CWDM","Fiber-pair","SM","1450nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C47-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1470nm ","SFP","CWDM","Fiber-pair","SM","1470nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C49-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1490nm ","SFP","CWDM","Fiber-pair","SM","1490nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C51-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1510nm ","SFP","CWDM","Fiber-pair","SM","1510nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C53-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1530nm ","SFP","CWDM","Fiber-pair","SM","1530nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C55-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1550nm ","SFP","CWDM","Fiber-pair","SM","1550nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C57-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1570nm ","SFP","CWDM","Fiber-pair","SM","1570nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C59-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1590nm ","SFP","CWDM","Fiber-pair","SM","1590nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-C61-E","SFP, 1G Ethernet, 1G FC, CWDM, 80km, 24dB, E-temp, LC, 1610nm ","SFP","CWDM","Fiber-pair","SM","1610nm","1GbE/1G FC","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D919","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D919","SFP","DWDM/100GHz","Fiber-pair","SM","D9190","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D920","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D920","SFP","DWDM/100GHz","Fiber-pair","SM","D9200","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D921","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D921","SFP","DWDM/100GHz","Fiber-pair","SM","D9210","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D922","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D922","SFP","DWDM/100GHz","Fiber-pair","SM","D9220","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D923","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D923","SFP","DWDM/100GHz","Fiber-pair","SM","D9230","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D924","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D924","SFP","DWDM/100GHz","Fiber-pair","SM","D9240","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D925","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D925","SFP","DWDM/100GHz","Fiber-pair","SM","D9250","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D926","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D926","SFP","DWDM/100GHz","Fiber-pair","SM","D9260","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D927","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D927","SFP","DWDM/100GHz","Fiber-pair","SM","D9270","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D928","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D928","SFP","DWDM/100GHz","Fiber-pair","SM","D9280","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D929","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D929","SFP","DWDM/100GHz","Fiber-pair","SM","D9290","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D930","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D930","SFP","DWDM/100GHz","Fiber-pair","SM","D9300","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D931","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D931","SFP","DWDM/100GHz","Fiber-pair","SM","D9310","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D932","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D932","SFP","DWDM/100GHz","Fiber-pair","SM","D9320","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D933","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D933","SFP","DWDM/100GHz","Fiber-pair","SM","D9330","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D934","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D934","SFP","DWDM/100GHz","Fiber-pair","SM","D9340","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D935","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D935","SFP","DWDM/100GHz","Fiber-pair","SM","D9350","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D936","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D936","SFP","DWDM/100GHz","Fiber-pair","SM","D9360","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D937","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D937","SFP","DWDM/100GHz","Fiber-pair","SM","D9370","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D938","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D938","SFP","DWDM/100GHz","Fiber-pair","SM","D9380","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D939","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D939","SFP","DWDM/100GHz","Fiber-pair","SM","D9390","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D940","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D940","SFP","DWDM/100GHz","Fiber-pair","SM","D9400","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D941","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D941","SFP","DWDM/100GHz","Fiber-pair","SM","D9410","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D942","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D942","SFP","DWDM/100GHz","Fiber-pair","SM","D9420","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D943","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D943","SFP","DWDM/100GHz","Fiber-pair","SM","D9430","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D944","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D944","SFP","DWDM/100GHz","Fiber-pair","SM","D9440","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D945","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D945","SFP","DWDM/100GHz","Fiber-pair","SM","D9450","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D946","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D946","SFP","DWDM/100GHz","Fiber-pair","SM","D9460","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D947","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D947","SFP","DWDM/100GHz","Fiber-pair","SM","D9470","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D948","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D948","SFP","DWDM/100GHz","Fiber-pair","SM","D9480","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D949","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D949","SFP","DWDM/100GHz","Fiber-pair","SM","D9490","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D950","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D950","SFP","DWDM/100GHz","Fiber-pair","SM","D9500","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D951","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D951","SFP","DWDM/100GHz","Fiber-pair","SM","D9510","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D952","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D952","SFP","DWDM/100GHz","Fiber-pair","SM","D9520","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D953","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D953","SFP","DWDM/100GHz","Fiber-pair","SM","D9530","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D954","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D954","SFP","DWDM/100GHz","Fiber-pair","SM","D9540","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D955","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D955","SFP","DWDM/100GHz","Fiber-pair","SM","D9550","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D956","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D956","SFP","DWDM/100GHz","Fiber-pair","SM","D9560","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D957","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D957","SFP","DWDM/100GHz","Fiber-pair","SM","D9570","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D958","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D958","SFP","DWDM/100GHz","Fiber-pair","SM","D9580","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D959","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D959","SFP","DWDM/100GHz","Fiber-pair","SM","D9590","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D960","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, LC, D960","SFP","DWDM/100GHz","Fiber-pair","SM","D9600","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-L80D-D919-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D919 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9190","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D920-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D920 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9200","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D921-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D921 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9210","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D922-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D922 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9220","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D923-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D923 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9230","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D924-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D924 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9240","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D925-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D925 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9250","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D926-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D926 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9260","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D927-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D927 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9270","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D928-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D928 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9280","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D929-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D929 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9290","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D930-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D930 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9300","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D931-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D931 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9310","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D932-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D932 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9320","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D933-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D933 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9330","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D934-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D934 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9340","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D935-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D935 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9350","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D936-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D936 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9360","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D937-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D937 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9370","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D938-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D938 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9380","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D939-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D939 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9390","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D940-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D940 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9400","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D941-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D941 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9410","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D942-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D942 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9420","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D943-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D943 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9430","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D944-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D944 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9440","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D945-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D945 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9450","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D946-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D946 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9460","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D947-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D947 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9470","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D948-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D948 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9480","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D949-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D949 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9490","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D950-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D950 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9500","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D951-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D951 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9510","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D952-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D952 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9520","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D953-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D953 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9530","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D954-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D954 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9540","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D955-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D955 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9550","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D956-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D956 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9560","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D957-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D957 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9570","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D958-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D958 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9580","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D959-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D959 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9590","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-L80D-D960-E","SFP, Multirate 0.1-1.25Gbps, DWDM 100GHz 80km, 28dB, E-temp, LC, D960 ","SFP","DWDM/100GHz","Fiber-pair","SM","D9600","1GbE/FE/1G FC/CPRI1/CPRI2/STM-4/OC-12/STM-1/OC3","80km","-","E-temp","Datasheet"]
[null,"SO-SFP-MR120D-C27","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C29","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C31","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C33","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C35","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C37","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C39","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C41","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C43","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C45","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C47","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C49","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C51","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C53","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C55","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C57","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C59","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-C61","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 33dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9210","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9210","SFP","DWDM/100GHz","Fiber-pair","SM","D9210","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9220","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9220","SFP","DWDM/100GHz","Fiber-pair","SM","D9220","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9230","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9230","SFP","DWDM/100GHz","Fiber-pair","SM","D9230","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9240","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9240","SFP","DWDM/100GHz","Fiber-pair","SM","D9240","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9250","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9250","SFP","DWDM/100GHz","Fiber-pair","SM","D9250","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9260","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9260","SFP","DWDM/100GHz","Fiber-pair","SM","D9260","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9270","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9270","SFP","DWDM/100GHz","Fiber-pair","SM","D9270","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9280","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9280","SFP","DWDM/100GHz","Fiber-pair","SM","D9280","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9290","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9290","SFP","DWDM/100GHz","Fiber-pair","SM","D9290","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9300","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9300","SFP","DWDM/100GHz","Fiber-pair","SM","D9300","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9310","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9310","SFP","DWDM/100GHz","Fiber-pair","SM","D9310","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9320","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9320","SFP","DWDM/100GHz","Fiber-pair","SM","D9320","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9330","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9330","SFP","DWDM/100GHz","Fiber-pair","SM","D9330","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9340","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9340","SFP","DWDM/100GHz","Fiber-pair","SM","D9340","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9350","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9350","SFP","DWDM/100GHz","Fiber-pair","SM","D9350","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9360","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9360","SFP","DWDM/100GHz","Fiber-pair","SM","D9360","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9370","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9370","SFP","DWDM/100GHz","Fiber-pair","SM","D9370","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9380","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9380","SFP","DWDM/100GHz","Fiber-pair","SM","D9380","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9390","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9390","SFP","DWDM/100GHz","Fiber-pair","SM","D9390","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9400","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9400","SFP","DWDM/100GHz","Fiber-pair","SM","D9400","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9410","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9410","SFP","DWDM/100GHz","Fiber-pair","SM","D9410","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9420","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9420","SFP","DWDM/100GHz","Fiber-pair","SM","D9420","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9430","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9430","SFP","DWDM/100GHz","Fiber-pair","SM","D9430","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9440","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9440","SFP","DWDM/100GHz","Fiber-pair","SM","D9440","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9450","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9450","SFP","DWDM/100GHz","Fiber-pair","SM","D9450","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9460","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9460","SFP","DWDM/100GHz","Fiber-pair","SM","D9460","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9470","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9470","SFP","DWDM/100GHz","Fiber-pair","SM","D9470","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9480","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9480","SFP","DWDM/100GHz","Fiber-pair","SM","D9480","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9490","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9490","SFP","DWDM/100GHz","Fiber-pair","SM","D9490","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9500","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9500","SFP","DWDM/100GHz","Fiber-pair","SM","D9500","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9510","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9510","SFP","DWDM/100GHz","Fiber-pair","SM","D9510","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9520","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9520","SFP","DWDM/100GHz","Fiber-pair","SM","D9520","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9530","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9530","SFP","DWDM/100GHz","Fiber-pair","SM","D9530","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9540","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9540","SFP","DWDM/100GHz","Fiber-pair","SM","D9540","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9550","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9550","SFP","DWDM/100GHz","Fiber-pair","SM","D9550","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9560","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9560","SFP","DWDM/100GHz","Fiber-pair","SM","D9560","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9570","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9570","SFP","DWDM/100GHz","Fiber-pair","SM","D9570","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9580","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9580","SFP","DWDM/100GHz","Fiber-pair","SM","D9580","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9590","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9590","SFP","DWDM/100GHz","Fiber-pair","SM","D9590","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR120D-D9600","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 120km, 33dB, LC, D9600","SFP","DWDM/100GHz","Fiber-pair","SM","D9600","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR15D","SFP, Multirate 100Mbps-2.7Gbps, SM 1310nm, 15km, 13dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","15km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR25-BX20D-34","SFP, BiDi, Multirate 100Mbps-2.7Gbps, TX/RX=1310/1490nm, SM, 20km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1310/1490nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR25-BX20D-43","SFP, BiDi, Multirate 100Mbps-2.7Gbps, TX/RX=1490/1310nm, SM, 20km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1490/1310nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","20km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR25-BX40D-35","SFP, BiDi, Multirate 100Mbps-2.7Gbps, TX/RX=1310/1550nm, SM, 40km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR25-BX40D-35-I","SFP, BiDi, Multirate 100Mbps-2.7Gbps, TX/RX=1310/1550nm, SM, 40km, 13dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1310/1550nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","40km","-","I-temp","Datasheet"]
[null,"SO-SFP-MR25-BX40D-53","SFP, BiDi, Multirate 100Mbps-2.7Gbps, TX/RX=1550/1310nm, SM, 40km, 13dB, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR25-BX40D-53-I","SFP, BiDi, Multirate 100Mbps-2.7Gbps, TX/RX=1550/1310nm, SM, 40km, 13dB, I-temp, LC","SFP","BiDi","Single-fiber","SM","1550/1310nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","40km","-","I-temp","Datasheet"]
[null,"SO-SFP-MR2D","SFP, Multirate 100Mbps-2.7Gbps, SM 1310nm, 2km, 8dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","2km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR40D","SFP, Multirate 100Mbps-2.7Gbps, SM 1310nm, 40km, 25dB, LC","SFP","Grey","Fiber-pair","SM","1310nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","40km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C27","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C29","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C31","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C33","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C35","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C37","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C39","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C41","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C43","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C45","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C47","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C49","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C51","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C53","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C55","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C57","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C59","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR50D-C61","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 17dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","50km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D","SFP, Multirate 100Mbps-2.7Gbps, SM 1550nm, 80km, 26dB, LC","SFP","Grey","Fiber-pair","SM","1550nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/1GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C27","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1270nm","SFP","CWDM","Fiber-pair","SM","1270nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C29","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1290nm","SFP","CWDM","Fiber-pair","SM","1290nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C31","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1310nm","SFP","CWDM","Fiber-pair","SM","1310nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C33","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1330nm","SFP","CWDM","Fiber-pair","SM","1330nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C35","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1350nm","SFP","CWDM","Fiber-pair","SM","1350nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C37","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1370nm","SFP","CWDM","Fiber-pair","SM","1370nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C39","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1390nm","SFP","CWDM","Fiber-pair","SM","1390nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C41","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1410nm","SFP","CWDM","Fiber-pair","SM","1410nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C43","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1430nm","SFP","CWDM","Fiber-pair","SM","1430nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C45","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1450nm","SFP","CWDM","Fiber-pair","SM","1450nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C47","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1470nm","SFP","CWDM","Fiber-pair","SM","1470nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C49","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1490nm","SFP","CWDM","Fiber-pair","SM","1490nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C51","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1510nm","SFP","CWDM","Fiber-pair","SM","1510nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C53","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1530nm","SFP","CWDM","Fiber-pair","SM","1530nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C55","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1550nm","SFP","CWDM","Fiber-pair","SM","1550nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C57","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1570nm","SFP","CWDM","Fiber-pair","SM","1570nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C59","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1590nm","SFP","CWDM","Fiber-pair","SM","1590nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-C61","SFP, Multirate 100Mbps-2.7Gbps, CWDM, 29dB, LC, 1610nm","SFP","CWDM","Fiber-pair","SM","1610nm","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9210","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9210","SFP","DWDM/100GHz","Fiber-pair","SM","D9210","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9220","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9220","SFP","DWDM/100GHz","Fiber-pair","SM","D9220","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9230","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9230","SFP","DWDM/100GHz","Fiber-pair","SM","D9230","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9240","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9240","SFP","DWDM/100GHz","Fiber-pair","SM","D9240","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9250","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9250","SFP","DWDM/100GHz","Fiber-pair","SM","D9250","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9260","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9260","SFP","DWDM/100GHz","Fiber-pair","SM","D9260","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9270","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9270","SFP","DWDM/100GHz","Fiber-pair","SM","D9270","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9280","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9280","SFP","DWDM/100GHz","Fiber-pair","SM","D9280","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9290","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9290","SFP","DWDM/100GHz","Fiber-pair","SM","D9290","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9300","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9300","SFP","DWDM/100GHz","Fiber-pair","SM","D9300","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9310","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9310","SFP","DWDM/100GHz","Fiber-pair","SM","D9310","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9320","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9320","SFP","DWDM/100GHz","Fiber-pair","SM","D9320","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9330","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9330","SFP","DWDM/100GHz","Fiber-pair","SM","D9330","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9340","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9340","SFP","DWDM/100GHz","Fiber-pair","SM","D9340","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9350","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9350","SFP","DWDM/100GHz","Fiber-pair","SM","D9350","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9360","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9360","SFP","DWDM/100GHz","Fiber-pair","SM","D9360","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9370","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9370","SFP","DWDM/100GHz","Fiber-pair","SM","D9370","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9380","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9380","SFP","DWDM/100GHz","Fiber-pair","SM","D9380","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9390","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9390","SFP","DWDM/100GHz","Fiber-pair","SM","D9390","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9400","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9400","SFP","DWDM/100GHz","Fiber-pair","SM","D9400","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9410","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9410","SFP","DWDM/100GHz","Fiber-pair","SM","D9410","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9420","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9420","SFP","DWDM/100GHz","Fiber-pair","SM","D9420","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9430","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9430","SFP","DWDM/100GHz","Fiber-pair","SM","D9430","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9440","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9440","SFP","DWDM/100GHz","Fiber-pair","SM","D9440","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9450","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9450","SFP","DWDM/100GHz","Fiber-pair","SM","D9450","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9460","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9460","SFP","DWDM/100GHz","Fiber-pair","SM","D9460","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9470","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9470","SFP","DWDM/100GHz","Fiber-pair","SM","D9470","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9480","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9480","SFP","DWDM/100GHz","Fiber-pair","SM","D9480","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9490","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9490","SFP","DWDM/100GHz","Fiber-pair","SM","D9490","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9500","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9500","SFP","DWDM/100GHz","Fiber-pair","SM","D9500","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9510","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9510","SFP","DWDM/100GHz","Fiber-pair","SM","D9510","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9520","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9520","SFP","DWDM/100GHz","Fiber-pair","SM","D9520","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9530","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9530","SFP","DWDM/100GHz","Fiber-pair","SM","D9530","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9540","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9540","SFP","DWDM/100GHz","Fiber-pair","SM","D9540","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9550","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9550","SFP","DWDM/100GHz","Fiber-pair","SM","D9550","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9560","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9560","SFP","DWDM/100GHz","Fiber-pair","SM","D9560","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9570","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9570","SFP","DWDM/100GHz","Fiber-pair","SM","D9570","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9580","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9580","SFP","DWDM/100GHz","Fiber-pair","SM","D9580","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9590","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9590","SFP","DWDM/100GHz","Fiber-pair","SM","D9590","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-MR80D-D9600","SFP, Multirate 100Mbps-2.7Gbps, DWDM 100GHz 80km, 29dB, LC, D9600","SFP","DWDM/100GHz","Fiber-pair","SM","D9600","STM16/OC-48/STM-4/OC-12/STM-1/OC-3/GbE/FE/2G FC/1G FC/OTU1/CPRI1/CPRI2/CPRI3","80km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX120D-5157","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1510/1570nm, SM, 120km, 33dB, LC","SFP","BiDi","Single-fiber","SM","1510/1570nm","1GbE/FE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX120D-5157-E","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1510/1570nm, SM, 120km, 33dB, E-temp, LC","SFP","BiDi","Single-fiber","SM","1510/1570nm","1GbE/FE/1G FC","120km","-","E-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX120D-5751","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1570/1510nm, SM, 120km, 33dB, LC","SFP","BiDi","Single-fiber","SM","1570/1510nm","1GbE/FE/1G FC","120km","-","C-temp","Datasheet"]
[null,"SO-SFP-1000Base-BX120D-5751-E","SFP, BiDi, 1G/100M Ethernet, 1G FC, TX/RX=1570/1510nm, SM, 120km, 33dB, E-temp, LC","SFP","BiDi","Single-fiber","SM","1570/1510nm","1GbE/FE/1G FC","120km","-","E-temp","Datasheet"]
[null,"16G-ER-BR2","SFP+, 16/8/4G FC, 1550nm, SM, 40km, 13dB, LC","SFP+","Grey","Fiber-pair","SM","1550nm","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D200-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D210-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D220-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D230-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D240-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D250-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D260-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D270-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D280-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D290-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D300-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D310-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D320-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D330-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D340-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D350-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D360-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D370-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D380-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D390-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D400-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D410-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D420-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D430-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D440-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D450-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D460-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D470-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D480-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D490-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D500-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D510-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D520-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D530-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D540-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D550-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D560-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D570-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D580-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D590-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D600-BR1","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 14dB, LC, D600","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D200-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D210-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D220-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D230-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D240-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D250-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D260-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D270-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D280-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D290-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D300-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D310-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D320-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D330-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D340-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D350-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D360-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D370-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D380-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D390-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D400-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D410-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D420-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D430-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D440-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D450-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D460-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D470-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D480-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D490-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D500-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D510-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D520-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D530-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D540-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D550-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D560-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D570-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D580-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D590-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D600-BR2","SFP+, 16/8/4G FC, DWDM 100GHz, 40km, 13dB, LC, D600","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D200-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D210-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D220-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D230-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D240-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D250-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D260-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D270-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D280-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D290-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D300-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D310-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D320-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D330-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D340-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D350-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D360-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D370-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D380-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D390-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D400-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D410-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D420-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D430-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D440-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D450-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D460-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D470-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D480-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D490-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D500-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D510-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D520-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D530-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D540-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D550-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D560-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D570-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D580-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D590-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ER-D600-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 40km, 14dB, LC, D600","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","8G FC/4G FC/2G FC","40km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-C47-BR1","SFP+, 8/4/2G FC, CWDM 70km, 23dB, LC, 1470nm","SFP+","CWDM","Fiber-pair","SM","1470nm","8G FC/4G FC/2G FC","70km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-C49-BR1","SFP+, 8/4/2G FC, CWDM 70km, 23dB, LC, 1490nm","SFP+","CWDM","Fiber-pair","SM","1490nm","8G FC/4G FC/2G FC","70km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-C51-BR1","SFP+, 8/4/2G FC, CWDM 70km, 23dB, LC, 1510nm","SFP+","CWDM","Fiber-pair","SM","1510nm","8G FC/4G FC/2G FC","70km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-C53-BR1","SFP+, 8/4/2G FC, CWDM 70km, 23dB, LC, 1530nm","SFP+","CWDM","Fiber-pair","SM","1530nm","8G FC/4G FC/2G FC","70km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-C55-BR1","SFP+, 8/4/2G FC, CWDM 70km, 23dB, LC, 1550nm","SFP+","CWDM","Fiber-pair","SM","1550nm","8G FC/4G FC/2G FC","70km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-C57-BR1","SFP+, 8/4/2G FC, CWDM 70km, 23dB, LC, 1570nm","SFP+","CWDM","Fiber-pair","SM","1570nm","8G FC/4G FC/2G FC","70km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-C59-BR1","SFP+, 8/4/2G FC, CWDM 70km, 23dB, LC, 1590nm","SFP+","CWDM","Fiber-pair","SM","1590nm","8G FC/4G FC/2G FC","70km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-C61-BR1","SFP+, 8/4/2G FC, CWDM 70km, 23dB, LC, 1610nm","SFP+","CWDM","Fiber-pair","SM","1610nm","8G FC/4G FC/2G FC","70km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D200-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D210-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D220-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D230-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D240-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D250-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D260-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D270-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D280-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D290-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D300-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D310-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D320-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D330-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D340-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D350-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D360-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D370-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D380-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D390-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D400-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D410-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D420-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D430-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D440-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D450-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D460-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D470-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D480-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D490-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D500-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D510-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D520-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D530-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D540-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D550-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D560-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D570-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D580-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D590-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"8G-ZR-D600-BR1","SFP+, 8/4/2G FC, DWDM 100GHz, 80km, 23dB, LC, D600","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","8G FC/4G FC/2G FC","80km","Brocade","C-temp","Datasheet"]
[null,"DS-16G-ER","SFP+, 16/8/4G FC, single channel 1550nm, SM, 40km, 13dB, LC","SFP+","Grey","Fiber-pair","SM","1550nm","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-C47","SFP+, 16/8/4G FC, CWDM, 40km, 13dB, LC, 1470nm","SFP+","CWDM","Fiber-pair","SM","1470nm","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-C49","SFP+, 16/8/4G FC, CWDM, 40km, 13dB, LC, 1490nm","SFP+","CWDM","Fiber-pair","SM","1490nm","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-C51","SFP+, 16/8/4G FC, CWDM, 40km, 13dB, LC, 1510nm","SFP+","CWDM","Fiber-pair","SM","1510nm","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-C53","SFP+, 16/8/4G FC, CWDM, 40km, 13dB, LC, 1530nm","SFP+","CWDM","Fiber-pair","SM","1530nm","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-C55","SFP+, 16/8/4G FC, CWDM, 40km, 13dB, LC, 1550nm","SFP+","CWDM","Fiber-pair","SM","1550nm","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D6142","SFP+, 16/8/4G FC, DWDM 100GHz, 192.00 THz, 40km, 13dB, LC, D6142","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D6061","SFP+, 16/8/4G FC, DWDM 100GHz, 192.10 THz, 40km, 13dB, LC, D6061","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5979","SFP+, 16/8/4G FC, DWDM 100GHz, 192.20 THz, 40km, 13dB, LC, D5979","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5898","SFP+, 16/8/4G FC, DWDM 100GHz, 192.30 THz, 40km, 13dB, LC, D5898","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5817","SFP+, 16/8/4G FC, DWDM 100GHz, 192.40 THz, 40km, 13dB, LC, D5817","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5736","SFP+, 16/8/4G FC, DWDM 100GHz, 192.50 THz, 40km, 13dB, LC, D5736","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5655","SFP+, 16/8/4G FC, DWDM 100GHz, 192.60 THz, 40km, 13dB, LC, D5655","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5575","SFP+, 16/8/4G FC, DWDM 100GHz, 192.70 THz, 40km, 13dB, LC, D5575","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5494","SFP+, 16/8/4G FC, DWDM 100GHz, 192.80 THz, 40km, 13dB, LC, D5494","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5413","SFP+, 16/8/4G FC, DWDM 100GHz, 192.90 THz, 40km, 13dB, LC, D5413","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5333","SFP+, 16/8/4G FC, DWDM 100GHz, 193.00 THz, 40km, 13dB, LC, D5333","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5252","SFP+, 16/8/4G FC, DWDM 100GHz, 193.10 THz, 40km, 13dB, LC, D5252","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5172","SFP+, 16/8/4G FC, DWDM 100GHz, 193.20 THz, 40km, 13dB, LC, D5172","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5092","SFP+, 16/8/4G FC, DWDM 100GHz, 193.30 THz, 40km, 13dB, LC, D5092","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D5012","SFP+, 16/8/4G FC, DWDM 100GHz, 193.40 THz, 40km, 13dB, LC, D5012","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4932","SFP+, 16/8/4G FC, DWDM 100GHz, 193.50 THz, 40km, 13dB, LC, D4932","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4851","SFP+, 16/8/4G FC, DWDM 100GHz, 193.60 THz, 40km, 13dB, LC, D4851","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4772","SFP+, 16/8/4G FC, DWDM 100GHz, 193.70 THz, 40km, 13dB, LC, D4772","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4692","SFP+, 16/8/4G FC, DWDM 100GHz, 193.80 THz, 40km, 13dB, LC, D4692","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4612","SFP+, 16/8/4G FC, DWDM 100GHz, 193.90 THz, 40km, 13dB, LC, D4612","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4532","SFP+, 16/8/4G FC, DWDM 100GHz, 194.00 THz, 40km, 13dB, LC, D4532","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4453","SFP+, 16/8/4G FC, DWDM 100GHz, 194.10 THz, 40km, 13dB, LC, D4453","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4373","SFP+, 16/8/4G FC, DWDM 100GHz, 194.20 THz, 40km, 13dB, LC, D4373","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4294","SFP+, 16/8/4G FC, DWDM 100GHz, 194.30 THz, 40km, 13dB, LC, D4294","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4214","SFP+, 16/8/4G FC, DWDM 100GHz, 194.40 THz, 40km, 13dB, LC, D4214","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4135","SFP+, 16/8/4G FC, DWDM 100GHz, 194.50 THz, 40km, 13dB, LC, D4135","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D4056","SFP+, 16/8/4G FC, DWDM 100GHz, 194.60 THz, 40km, 13dB, LC, D4056","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3977","SFP+, 16/8/4G FC, DWDM 100GHz, 194.70 THz, 40km, 13dB, LC, D3977","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3898","SFP+, 16/8/4G FC, DWDM 100GHz, 194.80 THz, 40km, 13dB, LC, D3898","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3819","SFP+, 16/8/4G FC, DWDM 100GHz, 194.90 THz, 40km, 13dB, LC, D3819","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3740","SFP+, 16/8/4G FC, DWDM 100GHz, 195.00 THz, 40km, 13dB, LC, D3740","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3661","SFP+, 16/8/4G FC, DWDM 100GHz, 195.10 THz, 40km, 13dB, LC, D3661","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3582","SFP+, 16/8/4G FC, DWDM 100GHz, 195.20 THz, 40km, 13dB, LC, D3582","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3504","SFP+, 16/8/4G FC, DWDM 100GHz, 195.30 THz, 40km, 13dB, LC, D3504","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3425","SFP+, 16/8/4G FC, DWDM 100GHz, 195.40 THz, 40km, 13dB, LC, D3425","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3347","SFP+, 16/8/4G FC, DWDM 100GHz, 195.50 THz, 40km, 13dB, LC, D3347","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3268","SFP+, 16/8/4G FC, DWDM 100GHz, 195.60 THz, 40km, 13dB, LC, D3268","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3190","SFP+, 16/8/4G FC, DWDM 100GHz, 195.70 THz, 40km, 13dB, LC, D3190","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3112","SFP+, 16/8/4G FC, DWDM 100GHz, 195.80 THz, 40km, 13dB, LC, D3112","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D3033","SFP+, 16/8/4G FC, DWDM 100GHz, 195.90 THz, 40km, 13dB, LC, D3033","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-16G-ER-D2955","SFP+, 16/8/4G FC, DWDM 100GHz, 196.00 THz, 40km, 13dB, LC, D2955","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","16G FC/8G FC/4G FC","40km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR","SFP+, 8/4/2G FC, single channel 1550nm, SM, 70km, 23dB, LC","SFP+","Grey","Fiber-pair","SM","1550nm","8G FC/4G FC/2G FC","70km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-C47","SFP+, 8/4/2G FC, CWDM, 70km, 23dB, LC, 1470nm","SFP+","CWDM","Fiber-pair","SM","1470nm","8G FC/4G FC/2G FC","70km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-C49","SFP+, 8/4/2G FC, CWDM, 70km, 23dB, LC, 1490nm","SFP+","CWDM","Fiber-pair","SM","1490nm","8G FC/4G FC/2G FC","70km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-C51","SFP+, 8/4/2G FC, CWDM, 70km, 23dB, LC, 1510nm","SFP+","CWDM","Fiber-pair","SM","1510nm","8G FC/4G FC/2G FC","70km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-C53","SFP+, 8/4/2G FC, CWDM, 70km, 23dB, LC, 1530nm","SFP+","CWDM","Fiber-pair","SM","1530nm","8G FC/4G FC/2G FC","70km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-C55","SFP+, 8/4/2G FC, CWDM, 70km, 23dB, LC, 1550nm","SFP+","CWDM","Fiber-pair","SM","1550nm","8G FC/4G FC/2G FC","70km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-C57","SFP+, 8/4/2G FC, CWDM, 70km, 23dB, LC, 1570nm","SFP+","CWDM","Fiber-pair","SM","1570nm","8G FC/4G FC/2G FC","70km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-C59","SFP+, 8/4/2G FC, CWDM, 70km, 23dB, LC, 1590nm","SFP+","CWDM","Fiber-pair","SM","1590nm","8G FC/4G FC/2G FC","70km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-C61","SFP+, 8/4/2G FC, CWDM, 70km, 23dB, LC, 1610nm","SFP+","CWDM","Fiber-pair","SM","1610nm","8G FC/4G FC/2G FC","70km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D6142","SFP+, 8/4/2G FC, DWDM 100GHz, 192.00 THz, 80km, 23dB, LC, D6142","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D6061","SFP+, 8/4/2G FC, DWDM 100GHz, 192.10 THz, 80km, 23dB, LC, D6061","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5979","SFP+, 8/4/2G FC, DWDM 100GHz, 192.20 THz, 80km, 23dB, LC, D5979","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5898","SFP+, 8/4/2G FC, DWDM 100GHz, 192.30 THz, 80km, 23dB, LC, D5898","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5817","SFP+, 8/4/2G FC, DWDM 100GHz, 192.40 THz, 80km, 23dB, LC, D5817","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5736","SFP+, 8/4/2G FC, DWDM 100GHz, 192.50 THz, 80km, 23dB, LC, D5736","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5655","SFP+, 8/4/2G FC, DWDM 100GHz, 192.60 THz, 80km, 23dB, LC, D5655","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5575","SFP+, 8/4/2G FC, DWDM 100GHz, 192.70 THz, 80km, 23dB, LC, D5575","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5494","SFP+, 8/4/2G FC, DWDM 100GHz, 192.80 THz, 80km, 23dB, LC, D5494","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5413","SFP+, 8/4/2G FC, DWDM 100GHz, 192.90 THz, 80km, 23dB, LC, D5413","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5333","SFP+, 8/4/2G FC, DWDM 100GHz, 193.00 THz, 80km, 23dB, LC, D5333","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5252","SFP+, 8/4/2G FC, DWDM 100GHz, 193.10 THz, 80km, 23dB, LC, D5252","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5172","SFP+, 8/4/2G FC, DWDM 100GHz, 193.20 THz, 80km, 23dB, LC, D5172","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5092","SFP+, 8/4/2G FC, DWDM 100GHz, 193.30 THz, 80km, 23dB, LC, D5092","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D5012","SFP+, 8/4/2G FC, DWDM 100GHz, 193.40 THz, 80km, 23dB, LC, D5012","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4932","SFP+, 8/4/2G FC, DWDM 100GHz, 193.50 THz, 80km, 23dB, LC, D4932","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4851","SFP+, 8/4/2G FC, DWDM 100GHz, 193.60 THz, 80km, 23dB, LC, D4851","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4772","SFP+, 8/4/2G FC, DWDM 100GHz, 193.70 THz, 80km, 23dB, LC, D4772","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4692","SFP+, 8/4/2G FC, DWDM 100GHz, 193.80 THz, 80km, 23dB, LC, D4692","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4612","SFP+, 8/4/2G FC, DWDM 100GHz, 193.90 THz, 80km, 23dB, LC, D4612","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4532","SFP+, 8/4/2G FC, DWDM 100GHz, 194.00 THz, 80km, 23dB, LC, D4532","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4453","SFP+, 8/4/2G FC, DWDM 100GHz, 194.10 THz, 80km, 23dB, LC, D4453","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4373","SFP+, 8/4/2G FC, DWDM 100GHz, 194.20 THz, 80km, 23dB, LC, D4373","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4294","SFP+, 8/4/2G FC, DWDM 100GHz, 194.30 THz, 80km, 23dB, LC, D4294","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4214","SFP+, 8/4/2G FC, DWDM 100GHz, 194.40 THz, 80km, 23dB, LC, D4214","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4135","SFP+, 8/4/2G FC, DWDM 100GHz, 194.50 THz, 80km, 23dB, LC, D4135","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D4056","SFP+, 8/4/2G FC, DWDM 100GHz, 194.60 THz, 80km, 23dB, LC, D4056","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3977","SFP+, 8/4/2G FC, DWDM 100GHz, 194.70 THz, 80km, 23dB, LC, D3977","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3898","SFP+, 8/4/2G FC, DWDM 100GHz, 194.80 THz, 80km, 23dB, LC, D3898","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3819","SFP+, 8/4/2G FC, DWDM 100GHz, 194.90 THz, 80km, 23dB, LC, D3819","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3740","SFP+, 8/4/2G FC, DWDM 100GHz, 195.00 THz, 80km, 23dB, LC, D3740","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3661","SFP+, 8/4/2G FC, DWDM 100GHz, 195.10 THz, 80km, 23dB, LC, D3661","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3582","SFP+, 8/4/2G FC, DWDM 100GHz, 195.20 THz, 80km, 23dB, LC, D3582","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3504","SFP+, 8/4/2G FC, DWDM 100GHz, 195.30 THz, 80km, 23dB, LC, D3504","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3425","SFP+, 8/4/2G FC, DWDM 100GHz, 195.40 THz, 80km, 23dB, LC, D3425","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3347","SFP+, 8/4/2G FC, DWDM 100GHz, 195.50 THz, 80km, 23dB, LC, D3347","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3268","SFP+, 8/4/2G FC, DWDM 100GHz, 195.60 THz, 80km, 23dB, LC, D3268","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3190","SFP+, 8/4/2G FC, DWDM 100GHz, 195.70 THz, 80km, 23dB, LC, D3190","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3112","SFP+, 8/4/2G FC, DWDM 100GHz, 195.80 THz, 80km, 23dB, LC, D3112","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D3033","SFP+, 8/4/2G FC, DWDM 100GHz, 195.90 THz, 80km, 23dB, LC, D3033","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"DS-8G-ZR-D2955","SFP+, 8/4/2G FC, DWDM 100GHz, 196.00 THz, 80km, 23dB, LC, D2955","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","8G FC/4G FC/2G FC","80km","Cisco","C-temp","Datasheet"]
[null,"SO-SFP-10GE-ACU1M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG30, Multirate 1Gbps to 10Gbps, 1m, active","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","1m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ACU3M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG30, Multirate 1Gbps to 10Gbps, 3m, active","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","3m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ACU5M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG28, Multirate 1Gbps to 10Gbps, 5m, active","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","5m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ACU7M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG28, Multirate 1Gbps to 10Gbps, 7m, active","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","7m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ACU10M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG24, Multirate 1Gbps to 10Gbps, 10m, active","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","10m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC1M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 1m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","1m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC2M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 2m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","2m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC3M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 3m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","3m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC4M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 4m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","4m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC5M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 5m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","5m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC6M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 6m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","6m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC7M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 7m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","7m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC8M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 8m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","8m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC9M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 9m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","9m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC10M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 10m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","10m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC15M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 15m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","15m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC20M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 20m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","20m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC30M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 30m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","30m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC50M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 50m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","50m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC70M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 70m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","70m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-AOC100M","SFP+ to SFP+, Active Optical Cable (AOC), MM, Multirate 4Gbps to 10Gbps, 100m","SFP+","AOC","Fiber-pair","MM","850nm","10GbE-LAN","100m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX10D-2733","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1270/1330nm, SM, 10km, 9dB, LC","SFP+","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX10D-2733-I","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1270/1330nm, SM, 10km, 9dB, I-temp, LC","SFP+","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-BX10D-3327","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1330/1270nm, SM, 10km, 9dB, LC","SFP+","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX10D-3327-I","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1330/1270nm, SM, 10km, 9dB, I-temp, LC","SFP+","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-BX20D-2733","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1270/1330nm, SM, 20km, 12dB, LC","SFP+","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","20km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX20D-2733-I","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1270/1330nm, SM, 20km, 12dB, I-temp, LC","SFP+","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","20km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-BX20D-3327","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1330/1270nm, SM, 20km, 12dB, LC","SFP+","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","20km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX20D-3327-I","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1330/1270nm, SM, 20km, 12dB, I-temp, LC","SFP+","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","20km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-BX40D-2733","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1270/1330nm, SM, 40km, 16dB, LC","SFP+","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX40D-2733-I","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1270/1330nm, SM, 40km, 16dB, I-temp, LC","SFP+","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-BX40D-3327","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1330/1270nm, SM, 40km, 16dB, LC","SFP+","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX40D-3327-I","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1330/1270nm, SM, 40km, 16dB, I-temp, LC","SFP+","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-BX60D-2733","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1270/1330nm, SM, 60km, 21dB, LC","SFP+","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","60km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX60D-2733-I","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1270/1330nm, SM, 60km, 21dB, I-temp, LC","SFP+","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","60km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-BX60D-3327","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1330/1270nm, SM, 60km, 21dB, LC","SFP+","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","60km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX60D-3327-I","SFP+, BiDi, 10G Multirate 0.6-11.3Gbps, Tx/Rx=1330/1270nm, SM, 60km, 21dB, I-temp, LC","SFP+","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","60km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-BX80D-4955","SFP+, BiDi, 10G Multirate 9.8-11.3Gbps, Tx/Rx=1490/1550nm, SM, 80km 22dB, LC","SFP+","BiDi","Single-fiber","SM","1490/1550nm","10GbE-LAN/10GbE-WAN/CPRI8/CPRI7","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-BX80D-5549","SFP+, BiDi, 10G Multirate 9.8-11.3Gbps, Tx/Rx=1550/1490nm, SM, 80km 22dB, LC","SFP+","BiDi","Single-fiber","SM","1550/1490nm","10GbE-LAN/10GbE-WAN/CPRI8/CPRI7","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-CU0.5M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG30, Multirate 1Gbps to 10Gbps, 0.5m, passive","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","0.5m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-CU1M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG30, Multirate 1Gbps to 10Gbps, 1m, passive","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","1m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-CU2M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG30, Multirate 1Gbps to 10Gbps, 2m, passive","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","2m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-CU3M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG30, Multirate 1Gbps to 10Gbps, 3m, passive","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","3m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-CU4M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG26, Multirate 1Gbps to 10Gbps, 4m, passive","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","4m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-CU5M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG26, Multirate 1Gbps to 10Gbps, 5m, passive","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","5m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-CU7M","SFP+ to SFP+, Direct Attach Cable (DAC), AWG24, Multirate 1Gbps to 10Gbps, 7m, passive","SFP+","DAC","Coax","Electrical",null,"10GbE-LAN/1GbE","7m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER","SFP+, 10G Multirate 0.6-11.3Gbps, SM, 1550nm, 40km, 11.1dB, LC","SFP+","Grey","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9200","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9205","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9205","SFP+","DWDM/100GHz","Fiber-pair","SM","D9205","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9210","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9215","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9215","SFP+","DWDM/100GHz","Fiber-pair","SM","D9215","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9220","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9225","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9225","SFP+","DWDM/100GHz","Fiber-pair","SM","D9225","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9230","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9235","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9235","SFP+","DWDM/100GHz","Fiber-pair","SM","D9235","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9240","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9245","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9245","SFP+","DWDM/100GHz","Fiber-pair","SM","D9245","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9250","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9255","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9255","SFP+","DWDM/100GHz","Fiber-pair","SM","D9255","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9260","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9265","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9265","SFP+","DWDM/100GHz","Fiber-pair","SM","D9265","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9270","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9275","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9275","SFP+","DWDM/100GHz","Fiber-pair","SM","D9275","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9280","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9285","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9285","SFP+","DWDM/100GHz","Fiber-pair","SM","D9285","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9290","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9295","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9295","SFP+","DWDM/100GHz","Fiber-pair","SM","D9295","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9300","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9305","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9305","SFP+","DWDM/100GHz","Fiber-pair","SM","D9305","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9310","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9315","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9315","SFP+","DWDM/100GHz","Fiber-pair","SM","D9315","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9320","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9325","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9325","SFP+","DWDM/100GHz","Fiber-pair","SM","D9325","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9330","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9335","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9335","SFP+","DWDM/100GHz","Fiber-pair","SM","D9335","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9340","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9345","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9345","SFP+","DWDM/100GHz","Fiber-pair","SM","D9345","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9350","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9355","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9355","SFP+","DWDM/100GHz","Fiber-pair","SM","D9355","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9360","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9365","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9365","SFP+","DWDM/100GHz","Fiber-pair","SM","D9365","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9370","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9375","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9375","SFP+","DWDM/100GHz","Fiber-pair","SM","D9375","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9380","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9385","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9385","SFP+","DWDM/100GHz","Fiber-pair","SM","D9385","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9390","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9395","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9395","SFP+","DWDM/100GHz","Fiber-pair","SM","D9395","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9400","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9405","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9405","SFP+","DWDM/100GHz","Fiber-pair","SM","D9405","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9410","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9415","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9415","SFP+","DWDM/100GHz","Fiber-pair","SM","D9415","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9420","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9425","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9425","SFP+","DWDM/100GHz","Fiber-pair","SM","D9425","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9430","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9435","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9435","SFP+","DWDM/100GHz","Fiber-pair","SM","D9435","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9440","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9445","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9445","SFP+","DWDM/100GHz","Fiber-pair","SM","D9445","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9450","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9455","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9455","SFP+","DWDM/100GHz","Fiber-pair","SM","D9455","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9460","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9465","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9465","SFP+","DWDM/100GHz","Fiber-pair","SM","D9465","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9470","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9475","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9475","SFP+","DWDM/100GHz","Fiber-pair","SM","D9475","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9480","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9485","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9485","SFP+","DWDM/100GHz","Fiber-pair","SM","D9485","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9490","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9495","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9495","SFP+","DWDM/100GHz","Fiber-pair","SM","D9495","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9500","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9505","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9505","SFP+","DWDM/100GHz","Fiber-pair","SM","D9505","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9510","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9515","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9515","SFP+","DWDM/100GHz","Fiber-pair","SM","D9515","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9520","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9525","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9525","SFP+","DWDM/100GHz","Fiber-pair","SM","D9525","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9530","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9535","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9535","SFP+","DWDM/100GHz","Fiber-pair","SM","D9535","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9540","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9545","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9545","SFP+","DWDM/100GHz","Fiber-pair","SM","D9545","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9550","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9555","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9555","SFP+","DWDM/100GHz","Fiber-pair","SM","D9555","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9560","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9565","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9565","SFP+","DWDM/100GHz","Fiber-pair","SM","D9565","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9570","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9575","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9575","SFP+","DWDM/100GHz","Fiber-pair","SM","D9575","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9580","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9585","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9585","SFP+","DWDM/100GHz","Fiber-pair","SM","D9585","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9590","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-50G-D9595","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz, 40km, 14dB, LC, D9595","SFP+","DWDM/100GHz","Fiber-pair","SM","D9595","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C47","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 15dB, LC, 1470nm","SFP+","CWDM","Fiber-pair","SM","1470nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C49","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 15dB, LC, 1490nm","SFP+","CWDM","Fiber-pair","SM","1490nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C51","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 15dB, LC, 1510nm","SFP+","CWDM","Fiber-pair","SM","1510nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C53","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 15dB, LC, 1530nm","SFP+","CWDM","Fiber-pair","SM","1530nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C55","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 15dB, LC, 1550nm","SFP+","CWDM","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C57","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 15dB, LC, 1570nm","SFP+","CWDM","Fiber-pair","SM","1570nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C59","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 15dB, LC, 1590nm","SFP+","CWDM","Fiber-pair","SM","1590nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C61","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 15dB, LC, 1610nm","SFP+","CWDM","Fiber-pair","SM","1610nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C47-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 14dB, E-temp, LC, 1470nm","SFP+","CWDM","Fiber-pair","SM","1470nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C49-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 14dB, E-temp, LC, 1490nm","SFP+","CWDM","Fiber-pair","SM","1490nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C51-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 14dB, E-temp, LC, 1510nm","SFP+","CWDM","Fiber-pair","SM","1510nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C53-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 14dB, E-temp, LC, 1530nm","SFP+","CWDM","Fiber-pair","SM","1530nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C55-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 14dB, E-temp, LC, 1550nm","SFP+","CWDM","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C57-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 14dB, E-temp, LC, 1570nm","SFP+","CWDM","Fiber-pair","SM","1570nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C59-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 14dB, E-temp, LC, 1590nm","SFP+","CWDM","Fiber-pair","SM","1590nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-C61-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 40km, 14dB, E-temp, LC, 1610nm","SFP+","CWDM","Fiber-pair","SM","1610nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9200","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9210","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9220","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9230","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9240","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9250","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9260","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9270","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9280","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9290","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9300","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9310","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9320","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9330","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9340","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9350","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9360","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9370","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9380","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9390","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9400","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9410","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9420","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9430","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9440","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9450","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9460","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9470","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9480","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9490","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9500","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9510","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9520","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9530","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9540","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9550","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9560","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9570","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9580","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9590","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9600","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 40km, 14dB, LC, D9600","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9200-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9200 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9210-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9210 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9220-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9220 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9230-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9230 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9240-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9240 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9250-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9250 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9260-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9260 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9270-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9270 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9280-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9280 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9290-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9290 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9300-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9300 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9310-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9310 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9320-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9320 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9330-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9330 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9340-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9340 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9350-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9350 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9360-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9360 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9370-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9370 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9380-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9380 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9390-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9390 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9400-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9400 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9410-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9410 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9420-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9420 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9430-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9430 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9440-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9440 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9450-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9450 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9460-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9460 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9470-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9470 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9480-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9480 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9490-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9490 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9500-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9500 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9510-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9510 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9520-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9520 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9530-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9530 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9540-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9540 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9550-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9550 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9560-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9560 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9570-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9570 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9580-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9580 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9590-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9590 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-D9600-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 40km 14dB I-temp LC D9600 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ER-I","SFP+, 10G Multirate 0.6-11.3Gbps, SM, 1550nm, 40km, 11.1dB, I-temp, LC","SFP+","Grey","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-LR","SFP+, 10G Multirate 0.6-11.3Gbps, SM, 1310nm, 10km, 6.2dB, LC","SFP+","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C27","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1270nm","SFP+","CWDM","Fiber-pair","SM","1270nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C29","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1290nm","SFP+","CWDM","Fiber-pair","SM","1290nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C31","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1310nm","SFP+","CWDM","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C33","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1330nm","SFP+","CWDM","Fiber-pair","SM","1330nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C35","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1350nm","SFP+","CWDM","Fiber-pair","SM","1350nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C37","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1370nm","SFP+","CWDM","Fiber-pair","SM","1370nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C39","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1390nm","SFP+","CWDM","Fiber-pair","SM","1390nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C41","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1410nm","SFP+","CWDM","Fiber-pair","SM","1410nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C43","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1430nm","SFP+","CWDM","Fiber-pair","SM","1430nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C45","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1450nm","SFP+","CWDM","Fiber-pair","SM","1450nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C47","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1470nm","SFP+","CWDM","Fiber-pair","SM","1470nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C49","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1490nm","SFP+","CWDM","Fiber-pair","SM","1490nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C51","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1510nm","SFP+","CWDM","Fiber-pair","SM","1510nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C53","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1530nm","SFP+","CWDM","Fiber-pair","SM","1530nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C55","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1550nm","SFP+","CWDM","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C57","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1570nm","SFP+","CWDM","Fiber-pair","SM","1570nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C59","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1590nm","SFP+","CWDM","Fiber-pair","SM","1590nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR10-C61","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 10km, 10dB, LC, 1610nm","SFP+","CWDM","Fiber-pair","SM","1610nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR20","SFP+, 10G Multirate 0.6-11.3Gbps, SM, 1310nm, 20km, 11.4dB, LC","SFP+","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","20km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR20-I","SFP+, 10G Multirate 0.6-11.3Gbps, SM, 1310nm, 20km, 11.4dB, I-temp, LC","SFP+","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","20km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C27","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1270nm","SFP+","CWDM","Fiber-pair","SM","1270nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C29","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1290nm","SFP+","CWDM","Fiber-pair","SM","1290nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C31","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1310nm","SFP+","CWDM","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C33","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1330nm","SFP+","CWDM","Fiber-pair","SM","1330nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C35","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1350nm","SFP+","CWDM","Fiber-pair","SM","1350nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C37","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1370nm","SFP+","CWDM","Fiber-pair","SM","1370nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C39","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1390nm","SFP+","CWDM","Fiber-pair","SM","1390nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C41","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1410nm","SFP+","CWDM","Fiber-pair","SM","1410nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C43","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1430nm","SFP+","CWDM","Fiber-pair","SM","1430nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40-C45","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 14dB, LC, 1450nm","SFP+","CWDM","Fiber-pair","SM","1450nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR-I","SFP+, 10G Multirate 0.6-11.3Gbps, SM, 1310nm, 10km, 6.2dB, I-temp, LC","SFP+","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","10km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-LRM","SFP+, 10G Multirate 0.6-11.3Gbps, MM, 1310nm, 220m@OM3, 3.5dB, LC","SFP+","Grey","Fiber-pair","MM","1310nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","220m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-LR40","SFP+, 10G Multirate 0.6-11.3Gbps, SM, 1310nm, 40km, 16dB, LC","SFP+","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","10GBASE-ER/-EW","C-temp","Datasheet"]
[null,"SO-SFP-10GE-SR","SFP+, 10G Multirate 0.6-11.3Gbps, MM 850nm, 300m@OM3, 5.1dB, LC","SFP+","Grey","Fiber-pair","MM","850nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","300m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-SR-I","SFP+, 10G Multirate 0.6-11.3Gbps, MM 850nm, 300m@OM3, 5.1dB, I-temp, LC","SFP+","Grey","Fiber-pair","MM","850nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","300m",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-T","SFP+, 10G Ethernet, 30m@CAT6A/CAT7, RJ45","SFP+","Grey","LAN","Electrical","-","10GbE-LAN","30m",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR","SFP+, 10G Multirate 0.6-11.3Gbps, 1550nm, SM, DDM, 23dB, 80km, LC","SFP+","Grey","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9200","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9205","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9205","SFP+","DWDM/100GHz","Fiber-pair","SM","D9205","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9210","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9215","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9215","SFP+","DWDM/100GHz","Fiber-pair","SM","D9215","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9220","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9225","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9225","SFP+","DWDM/100GHz","Fiber-pair","SM","D9225","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9230","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9235","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9235","SFP+","DWDM/100GHz","Fiber-pair","SM","D9235","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9240","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9245","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9245","SFP+","DWDM/100GHz","Fiber-pair","SM","D9245","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9250","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9255","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9255","SFP+","DWDM/100GHz","Fiber-pair","SM","D9255","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9260","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9265","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9265","SFP+","DWDM/100GHz","Fiber-pair","SM","D9265","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9270","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9275","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9275","SFP+","DWDM/100GHz","Fiber-pair","SM","D9275","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9280","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9285","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9285","SFP+","DWDM/100GHz","Fiber-pair","SM","D9285","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9290","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9295","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9295","SFP+","DWDM/100GHz","Fiber-pair","SM","D9295","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9300","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9305","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9305","SFP+","DWDM/100GHz","Fiber-pair","SM","D9305","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9310","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9315","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9315","SFP+","DWDM/100GHz","Fiber-pair","SM","D9315","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9320","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9325","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9325","SFP+","DWDM/100GHz","Fiber-pair","SM","D9325","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9330","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9335","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9335","SFP+","DWDM/100GHz","Fiber-pair","SM","D9335","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9340","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9345","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9345","SFP+","DWDM/100GHz","Fiber-pair","SM","D9345","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9350","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9355","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9355","SFP+","DWDM/100GHz","Fiber-pair","SM","D9355","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9360","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9365","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9365","SFP+","DWDM/100GHz","Fiber-pair","SM","D9365","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9370","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9375","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9375","SFP+","DWDM/100GHz","Fiber-pair","SM","D9375","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9380","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9385","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9385","SFP+","DWDM/100GHz","Fiber-pair","SM","D9385","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9390","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9395","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9395","SFP+","DWDM/100GHz","Fiber-pair","SM","D9395","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9400","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9405","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9405","SFP+","DWDM/100GHz","Fiber-pair","SM","D9405","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9410","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9415","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9415","SFP+","DWDM/100GHz","Fiber-pair","SM","D9415","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9420","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9425","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9425","SFP+","DWDM/100GHz","Fiber-pair","SM","D9425","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9430","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9435","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9435","SFP+","DWDM/100GHz","Fiber-pair","SM","D9435","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9440","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9445","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9445","SFP+","DWDM/100GHz","Fiber-pair","SM","D9445","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9450","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9455","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9455","SFP+","DWDM/100GHz","Fiber-pair","SM","D9455","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9460","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9465","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9465","SFP+","DWDM/100GHz","Fiber-pair","SM","D9465","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9470","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9475","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9475","SFP+","DWDM/100GHz","Fiber-pair","SM","D9475","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9480","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9485","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9485","SFP+","DWDM/100GHz","Fiber-pair","SM","D9485","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9490","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9495","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9495","SFP+","DWDM/100GHz","Fiber-pair","SM","D9495","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9500","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9505","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9505","SFP+","DWDM/100GHz","Fiber-pair","SM","D9505","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9510","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9515","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9515","SFP+","DWDM/100GHz","Fiber-pair","SM","D9515","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9520","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9525","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9525","SFP+","DWDM/100GHz","Fiber-pair","SM","D9525","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9530","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9535","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9535","SFP+","DWDM/100GHz","Fiber-pair","SM","D9535","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9540","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9545","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9545","SFP+","DWDM/100GHz","Fiber-pair","SM","D9545","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9550","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9555","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9555","SFP+","DWDM/100GHz","Fiber-pair","SM","D9555","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9560","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9565","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9565","SFP+","DWDM/100GHz","Fiber-pair","SM","D9565","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9570","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9575","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9575","SFP+","DWDM/100GHz","Fiber-pair","SM","D9575","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9580","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9585","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9585","SFP+","DWDM/100GHz","Fiber-pair","SM","D9585","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9590","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-50G-D9595","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 50GHz 80km, 23dB, LC, D9595","SFP+","DWDM/100GHz","Fiber-pair","SM","D9595","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C47","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, LC, 1470nm","SFP+","CWDM","Fiber-pair","SM","1470nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C49","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, LC, 1490nm","SFP+","CWDM","Fiber-pair","SM","1490nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C51","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, LC, 1510nm","SFP+","CWDM","Fiber-pair","SM","1510nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C53","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, LC, 1530nm","SFP+","CWDM","Fiber-pair","SM","1530nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C55","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, LC, 1550nm","SFP+","CWDM","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C57","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, LC, 1570nm","SFP+","CWDM","Fiber-pair","SM","1570nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C59","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, LC, 1590nm","SFP+","CWDM","Fiber-pair","SM","1590nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C61","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, LC, 1610nm","SFP+","CWDM","Fiber-pair","SM","1610nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C47-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, E-temp, LC, 1470nm","SFP+","CWDM","Fiber-pair","SM","1470nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C49-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, E-temp, LC, 1490nm","SFP+","CWDM","Fiber-pair","SM","1490nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C51-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, E-temp, LC, 1510nm","SFP+","CWDM","Fiber-pair","SM","1510nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C53-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, E-temp, LC, 1530nm","SFP+","CWDM","Fiber-pair","SM","1530nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C55-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, E-temp, LC, 1550nm","SFP+","CWDM","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C57-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, E-temp, LC, 1570nm","SFP+","CWDM","Fiber-pair","SM","1570nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C59-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, E-temp, LC, 1590nm","SFP+","CWDM","Fiber-pair","SM","1590nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-C61-E","SFP+, 10G Multirate 0.6-11.3Gbps, CWDM, 80km, 23dB, E-temp, LC, 1610nm","SFP+","CWDM","Fiber-pair","SM","1610nm","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"E-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9200","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9210","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9220","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9230","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9240","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9250","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9260","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9270","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9280","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9290","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9300","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9310","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz, 80km, 23dB, LC, D9310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9320","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9330","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9340","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9350","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9360","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9370","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9380","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9390","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9400","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9410","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9420","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9430","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9440","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9450","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9460","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9470","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9480","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9490","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9500","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9510","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9520","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9530","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9540","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9550","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9560","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9570","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9580","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9590","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9600","SFP+, 10G Multirate 0.6-11.3Gbps, DWDM 100GHz 80km, 23dB, LC, D9600","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9200-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9200 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9210-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9210 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9220-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9220 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9230-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9230 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9240-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9240 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9250-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9250 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9260-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9260 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9270-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9270 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9280-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9280 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9290-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9290 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9300-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9300 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9310-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9310 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9320-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9320 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9330-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9330 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9340-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9340 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9350-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9350 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9360-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9360 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9370-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9370 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9380-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9380 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9390-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9390 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9400-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9400 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9410-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9410 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9420-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9420 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9430-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9430 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9440-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9440 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9450-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9450 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9460-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9460 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9470-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9470 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9480-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9480 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9490-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9490 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9500-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9500 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9510-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9510 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9520-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9520 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9530-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9530 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9540-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9540 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9550-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9550 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9560-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9560 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9570-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9570 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9580-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9580 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9590-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9590 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-D9600-I","SFP+ 10G Multirate 0.6-11.3Gbps DWDM 100GHz 80km 23dB I-temp LC D9600 ","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","10GbE-LAN/10GbE-WAN/GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10GE-ZR-I","SFP+, 10G Multirate 0.6-11.3Gbps, 1550nm, SM, DDM, 23dB, 80km, I-temp, LC","SFP+","Grey","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP-10G-ZR100","SFP+, 10G Multirate 0.6-11.3Gbps, 1550nm, SM, DDM, 26dB, 100km, LC","SFP+","Grey","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/STM-4/OC-12/10G FC/8G FC/4G FC/1G FC/CPRI1/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","100km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-C47","SFP+, 16/8/4G FC, CWDM 40km, 13dB, LC, 1470nm","SFP+","CWDM","Fiber-pair","SM","1470nm","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-C49","SFP+, 16/8/4G FC, CWDM 40km, 13dB, LC, 1490nm","SFP+","CWDM","Fiber-pair","SM","1490nm","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-C51","SFP+, 16/8/4G FC, CWDM 40km, 13dB, LC, 1510nm","SFP+","CWDM","Fiber-pair","SM","1510nm","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-C53","SFP+, 16/8/4G FC, CWDM 40km, 13dB, LC, 1530nm","SFP+","CWDM","Fiber-pair","SM","1530nm","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-C55","SFP+, 16/8/4G FC, CWDM 40km, 13dB, LC, 1550nm","SFP+","CWDM","Fiber-pair","SM","1550nm","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9200","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9210","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9220","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9230","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9240","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9250","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9260","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9270","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9280","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9290","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9300","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9310","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9320","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9330","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9340","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9350","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9360","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9370","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9380","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9390","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9400","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9410","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9420","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9430","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9440","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9450","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9460","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9470","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9480","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9490","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9500","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9510","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9520","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9530","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9540","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9550","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9560","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9570","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9580","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9590","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-ER-D9600","SFP+, 16/8/4G FC, DWDM 100GHz grid, 40km, 14dB, LC, D9600","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","16G FC/8G FC/4G FC","40km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-LD","SFP+, 16G/8G/4G FC, SM 1310nm, 10km, 6.9dB, LC","SFP+","Grey","Fiber-pair","SM","1310nm","16G FC/8G FC/4G FC","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-16GFC-SD","SFP+, 16G/8G/4G FC, MM 850nm, 100m@OM3, 150m@OM4, 4.2dB, LC","SFP+","Grey","Fiber-pair","MM","850nm","16G FC/8G FC/4G FC","150m",null,"C-temp","Datasheet"]
[null,"SO-SFP-1G-10G-LR","SFP+, 1G/10G Ethernet SR, 10G SDH/SONET, SM 1310nm, 10km, 6.2dB@10G, 11.5dB@1G, LC","SFP+","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/1GbE/STM-64/OC-192","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-1G-10G-SR","SFP+, 1G/10G Ethernet SR, 10G SDH/SONET, MM 850nm, 300m, 5.1dB@10G, 7.5dB@1G, LC","SFP+","Grey","Fiber-pair","MM","850nm","10GbE-LAN/10GbE-WAN/1GbE/STM-64/OC-192","300m",null,"C-temp","Datasheet"]
[null,"SO-SFP-8GFC-L10D","SFP+, 8G/4G/2G/1G FC, Multirate 614Mbps-8.5Gbps SM 1310nm, 10km, 6.8dB, LC","SFP+","Grey","Fiber-pair","SM","1310nm","8G FC/4G FC/2G FC/1G FC/1GbE","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP-8GFC-SD","SFP+, 8G/4G/2G/1G FC, Multirate 614Mbps-8.5Gbps MM 850nm, 300m@OM3, 5.1dB, LC","SFP+","Grey","Fiber-pair","MM","850nm","8G FC/4G FC/2G FC/1G FC","300m",null,"C-temp","Datasheet"]
[null,"SO-TSFP10GER-D1I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Tunable D920-928 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D920-928","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP10GER-D2I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Tunable D928-936 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D928-936","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP10GER-D3I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Tunable D936-944 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D936-944","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP10GER-D4I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Tunable D944-952 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D944-952","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP10GER-D5I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Tunable D952-960 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D952-960","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP10GER-A1I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Auto Tunable D920-928 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D920-928","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP10GER-A2I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Auto Tunable D928-936 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D928-936","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP10GER-A3I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Auto Tunable D936-944 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D936-944","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP10GER-A4I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Auto Tunable D944-952 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D944-952","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP10GER-A5I","SFP+ 10G Multirate 1.0-11.3Gbps DWDM 100GHz 40km 22dB Auto Tunable D952-960 I-temp LC","SFP+","DWDM/100GHz-Tune","Fiber-pair","SM","D952-960","10GbE-LAN/10GbE-WAN/1GbE/OTU2e/OTU2/OTU1/STM-64/OC-192/STM16/OC-48/10G FC/8G FC/4G FC/1G FC/CPRI2/CPRI3/CPRI4/CPRI5/CPRI6/CPRI7/CPRI-7A/CPRI8","40km","-","I-temp","Datasheet"]
[null,"SO-TSFP-10G-ZR-DWDM-A","SFP+, 10G Multirate 9.95-11.3Gbps, DWDM 50GHz Tunable 191.35-196.10THz (96ch), 80km, 23dB, LC","SFP+","DWDM/50GHz-Tune","Fiber-pair","SM","D9135 - D9610","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-TSFP-10G-ZR-DWDM-I","SFP+ 10G Multirate 1.2-11.3Gbps DWDM 50GHz Tunable 191.35-196.10THz (96ch) 80km 23dB I-temp LC","SFP+","DWDM/50GHz-Tune","Fiber-pair","SM","D9135 - D9610","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"I-temp","Datasheet"]
[null,"SO-SFP28-PCU0.5M","SFP28 to SFP28 Direct Attach Cable (DAC), 25G Ethernet, AWG30, 0.5m, passive","SFP28","DAC","Coax","Electrical","-","25GE","0.5m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-PCU1M","SFP28 to SFP28 Direct Attach Cable (DAC), 25G Ethernet, AWG30, 1m, passive","SFP28","DAC","Coax","Electrical","-","25GE","1m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-PCU2M","SFP28 to SFP28 Direct Attach Cable (DAC), 25G Ethernet, AWG30, 2m, passive","SFP28","DAC","Coax","Electrical","-","25GE","2m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-PCU3M","SFP28 to SFP28 Direct Attach Cable (DAC), 25G Ethernet, AWG30, 3m, passive","SFP28","DAC","Coax","Electrical","-","25GE","3m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-PCU5M","SFP28 to SFP28 Direct Attach Cable (DAC), 25G Ethernet, AWG26, 5m, passive","SFP28","DAC","Coax","Electrical","-","25GE","5m",null,"C-temp","Datasheet"]
[null,"32G-IR-D200-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D200","SFP28","DWDM/100GHz","Fiber-pair","SM","D9200","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D210-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D210","SFP28","DWDM/100GHz","Fiber-pair","SM","D9210","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D220-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D220","SFP28","DWDM/100GHz","Fiber-pair","SM","D9220","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D230-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D230","SFP28","DWDM/100GHz","Fiber-pair","SM","D9230","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D240-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D240","SFP28","DWDM/100GHz","Fiber-pair","SM","D9240","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D250-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D250","SFP28","DWDM/100GHz","Fiber-pair","SM","D9250","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D260-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D260","SFP28","DWDM/100GHz","Fiber-pair","SM","D9260","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D270-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D270","SFP28","DWDM/100GHz","Fiber-pair","SM","D9270","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D280-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D280","SFP28","DWDM/100GHz","Fiber-pair","SM","D9280","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D290-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D290","SFP28","DWDM/100GHz","Fiber-pair","SM","D9290","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D300-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D300","SFP28","DWDM/100GHz","Fiber-pair","SM","D9300","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D310-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D310","SFP28","DWDM/100GHz","Fiber-pair","SM","D9310","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D320-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D320","SFP28","DWDM/100GHz","Fiber-pair","SM","D9320","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D330-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D330","SFP28","DWDM/100GHz","Fiber-pair","SM","D9330","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D340-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D340","SFP28","DWDM/100GHz","Fiber-pair","SM","D9340","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D350-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D350","SFP28","DWDM/100GHz","Fiber-pair","SM","D9350","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D360-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D360","SFP28","DWDM/100GHz","Fiber-pair","SM","D9360","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D370-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D370","SFP28","DWDM/100GHz","Fiber-pair","SM","D9370","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D380-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D380","SFP28","DWDM/100GHz","Fiber-pair","SM","D9380","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D390-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D390","SFP28","DWDM/100GHz","Fiber-pair","SM","D9390","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D400-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D400","SFP28","DWDM/100GHz","Fiber-pair","SM","D9400","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D410-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D410","SFP28","DWDM/100GHz","Fiber-pair","SM","D9410","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D420-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D420","SFP28","DWDM/100GHz","Fiber-pair","SM","D9420","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D430-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D430","SFP28","DWDM/100GHz","Fiber-pair","SM","D9430","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D440-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D440","SFP28","DWDM/100GHz","Fiber-pair","SM","D9440","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D450-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D450","SFP28","DWDM/100GHz","Fiber-pair","SM","D9450","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D460-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D460","SFP28","DWDM/100GHz","Fiber-pair","SM","D9460","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D470-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D470","SFP28","DWDM/100GHz","Fiber-pair","SM","D9470","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D480-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D480","SFP28","DWDM/100GHz","Fiber-pair","SM","D9480","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D490-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D490","SFP28","DWDM/100GHz","Fiber-pair","SM","D9490","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D500-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D500","SFP28","DWDM/100GHz","Fiber-pair","SM","D9500","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D510-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D510","SFP28","DWDM/100GHz","Fiber-pair","SM","D9510","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D520-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D520","SFP28","DWDM/100GHz","Fiber-pair","SM","D9520","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D530-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D530","SFP28","DWDM/100GHz","Fiber-pair","SM","D9530","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D540-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D540","SFP28","DWDM/100GHz","Fiber-pair","SM","D9540","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D550-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D550","SFP28","DWDM/100GHz","Fiber-pair","SM","D9550","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D560-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D560","SFP28","DWDM/100GHz","Fiber-pair","SM","D9560","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D570-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D570","SFP28","DWDM/100GHz","Fiber-pair","SM","D9570","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D580-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D580","SFP28","DWDM/100GHz","Fiber-pair","SM","D9580","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D590-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D590","SFP28","DWDM/100GHz","Fiber-pair","SM","D9590","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D600-BR","SFP28, 32/16/8G FC, DWDM 100GHz, 10km, 7dB, LC, D600","SFP28","DWDM/100GHz","Fiber-pair","SM","D9600","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"DS-32G-IR-D6142","SFP28, 32/16/8G FC, DWDM 100GHz 192.00 THz, 10km, 7dB, LC, D6142","SFP28","DWDM/100GHz","Fiber-pair","SM","D9200","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D6061","SFP28, 32/16/8G FC, DWDM 100GHz 192.10 THz, 10km, 7dB, LC, D6061","SFP28","DWDM/100GHz","Fiber-pair","SM","D9210","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5979","SFP28, 32/16/8G FC, DWDM 100GHz 192.20 THz, 10km, 7dB, LC, D5979","SFP28","DWDM/100GHz","Fiber-pair","SM","D9220","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5898","SFP28, 32/16/8G FC, DWDM 100GHz 192.30 THz, 10km, 7dB, LC, D5898","SFP28","DWDM/100GHz","Fiber-pair","SM","D9230","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5817","SFP28, 32/16/8G FC, DWDM 100GHz 192.40 THz, 10km, 7dB, LC, D5817","SFP28","DWDM/100GHz","Fiber-pair","SM","D9240","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5736","SFP28, 32/16/8G FC, DWDM 100GHz 192.50 THz, 10km, 7dB, LC, D5736","SFP28","DWDM/100GHz","Fiber-pair","SM","D9250","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5655","SFP28, 32/16/8G FC, DWDM 100GHz 192.60 THz, 10km, 7dB, LC, D5655","SFP28","DWDM/100GHz","Fiber-pair","SM","D9260","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5575","SFP28, 32/16/8G FC, DWDM 100GHz 192.70 THz, 10km, 7dB, LC, D5575","SFP28","DWDM/100GHz","Fiber-pair","SM","D9270","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5494","SFP28, 32/16/8G FC, DWDM 100GHz 192.80 THz, 10km, 7dB, LC, D5494","SFP28","DWDM/100GHz","Fiber-pair","SM","D9280","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5413","SFP28, 32/16/8G FC, DWDM 100GHz 192.90 THz, 10km, 7dB, LC, D5413","SFP28","DWDM/100GHz","Fiber-pair","SM","D9290","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5333","SFP28, 32/16/8G FC, DWDM 100GHz 193.00 THz, 10km, 7dB, LC, D5333","SFP28","DWDM/100GHz","Fiber-pair","SM","D9300","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5252","SFP28, 32/16/8G FC, DWDM 100GHz 193.10 THz, 10km, 7dB, LC, D5252","SFP28","DWDM/100GHz","Fiber-pair","SM","D9310","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5172","SFP28, 32/16/8G FC, DWDM 100GHz 193.20 THz, 10km, 7dB, LC, D5172","SFP28","DWDM/100GHz","Fiber-pair","SM","D9320","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5092","SFP28, 32/16/8G FC, DWDM 100GHz 193.30 THz, 10km, 7dB, LC, D5092","SFP28","DWDM/100GHz","Fiber-pair","SM","D9330","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D5012","SFP28, 32/16/8G FC, DWDM 100GHz 193.40 THz, 10km, 7dB, LC, D5012","SFP28","DWDM/100GHz","Fiber-pair","SM","D9340","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4932","SFP28, 32/16/8G FC, DWDM 100GHz 193.50 THz, 10km, 7dB, LC, D4932","SFP28","DWDM/100GHz","Fiber-pair","SM","D9350","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4851","SFP28, 32/16/8G FC, DWDM 100GHz 193.60 THz, 10km, 7dB, LC, D4851","SFP28","DWDM/100GHz","Fiber-pair","SM","D9360","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4772","SFP28, 32/16/8G FC, DWDM 100GHz 193.70 THz, 10km, 7dB, LC, D4772","SFP28","DWDM/100GHz","Fiber-pair","SM","D9370","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4692","SFP28, 32/16/8G FC, DWDM 100GHz 193.80 THz, 10km, 7dB, LC, D4692","SFP28","DWDM/100GHz","Fiber-pair","SM","D9380","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4612","SFP28, 32/16/8G FC, DWDM 100GHz 193.90 THz, 10km, 7dB, LC, D4612","SFP28","DWDM/100GHz","Fiber-pair","SM","D9390","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4532","SFP28, 32/16/8G FC, DWDM 100GHz 194.00 THz, 10km, 7dB, LC, D4532","SFP28","DWDM/100GHz","Fiber-pair","SM","D9400","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4453","SFP28, 32/16/8G FC, DWDM 100GHz 194.10 THz, 10km, 7dB, LC, D4453","SFP28","DWDM/100GHz","Fiber-pair","SM","D9410","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4373","SFP28, 32/16/8G FC, DWDM 100GHz 194.20 THz, 10km, 7dB, LC, D4373","SFP28","DWDM/100GHz","Fiber-pair","SM","D9420","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4294","SFP28, 32/16/8G FC, DWDM 100GHz 194.30 THz, 10km, 7dB, LC, D4294","SFP28","DWDM/100GHz","Fiber-pair","SM","D9430","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4214","SFP28, 32/16/8G FC, DWDM 100GHz 194.40 THz, 10km, 7dB, LC, D4214","SFP28","DWDM/100GHz","Fiber-pair","SM","D9440","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4135","SFP28, 32/16/8G FC, DWDM 100GHz 194.50 THz, 10km, 7dB, LC, D4135","SFP28","DWDM/100GHz","Fiber-pair","SM","D9450","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D4056","SFP28, 32/16/8G FC, DWDM 100GHz 194.60 THz, 10km, 7dB, LC, D4056","SFP28","DWDM/100GHz","Fiber-pair","SM","D9460","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3977","SFP28, 32/16/8G FC, DWDM 100GHz 194.70 THz, 10km, 7dB, LC, D3977","SFP28","DWDM/100GHz","Fiber-pair","SM","D9470","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3898","SFP28, 32/16/8G FC, DWDM 100GHz 194.80 THz, 10km, 7dB, LC, D3898","SFP28","DWDM/100GHz","Fiber-pair","SM","D9480","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3819","SFP28, 32/16/8G FC, DWDM 100GHz 194.90 THz, 10km, 7dB, LC, D3819","SFP28","DWDM/100GHz","Fiber-pair","SM","D9490","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3740","SFP28, 32/16/8G FC, DWDM 100GHz 195.00 THz, 10km, 7dB, LC, D3740","SFP28","DWDM/100GHz","Fiber-pair","SM","D9500","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3661","SFP28, 32/16/8G FC, DWDM 100GHz 195.10 THz, 10km, 7dB, LC, D3661","SFP28","DWDM/100GHz","Fiber-pair","SM","D9510","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3582","SFP28, 32/16/8G FC, DWDM 100GHz 195.20 THz, 10km, 7dB, LC, D3582","SFP28","DWDM/100GHz","Fiber-pair","SM","D9520","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3504","SFP28, 32/16/8G FC, DWDM 100GHz 195.30 THz, 10km, 7dB, LC, D3504","SFP28","DWDM/100GHz","Fiber-pair","SM","D9530","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3425","SFP28, 32/16/8G FC, DWDM 100GHz 195.40 THz, 10km, 7dB, LC, D3425","SFP28","DWDM/100GHz","Fiber-pair","SM","D9540","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3347","SFP28, 32/16/8G FC, DWDM 100GHz 195.50 THz, 10km, 7dB, LC, D3347","SFP28","DWDM/100GHz","Fiber-pair","SM","D9550","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3268","SFP28, 32/16/8G FC, DWDM 100GHz 195.60 THz, 10km, 7dB, LC, D3268","SFP28","DWDM/100GHz","Fiber-pair","SM","D9560","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3190","SFP28, 32/16/8G FC, DWDM 100GHz 195.70 THz, 10km, 7dB, LC, D3190","SFP28","DWDM/100GHz","Fiber-pair","SM","D9570","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3112","SFP28, 32/16/8G FC, DWDM 100GHz 195.80 THz, 10km, 7dB, LC, D3112","SFP28","DWDM/100GHz","Fiber-pair","SM","D9580","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D3033","SFP28, 32/16/8G FC, DWDM 100GHz 195.90 THz, 10km, 7dB, LC, D3033","SFP28","DWDM/100GHz","Fiber-pair","SM","D9590","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"DS-32G-IR-D2955","SFP28, 32/16/8G FC, DWDM 100GHz 196.00 THz, 10km, 7dB, LC, D2955","SFP28","DWDM/100GHz","Fiber-pair","SM","D9600","16G FC/8G FC/4G FC","10km","Cisco","C-temp","Datasheet"]
[null,"32G-IR-D20S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D200","SFP28","DWDM/100GHz","Fiber-pair","SM","D9200","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D21S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D210","SFP28","DWDM/100GHz","Fiber-pair","SM","D9210","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D22S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D220","SFP28","DWDM/100GHz","Fiber-pair","SM","D9220","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D23S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D230","SFP28","DWDM/100GHz","Fiber-pair","SM","D9230","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D24S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D240","SFP28","DWDM/100GHz","Fiber-pair","SM","D9240","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D25S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D250","SFP28","DWDM/100GHz","Fiber-pair","SM","D9250","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D26S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D260","SFP28","DWDM/100GHz","Fiber-pair","SM","D9260","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D27S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D270","SFP28","DWDM/100GHz","Fiber-pair","SM","D9270","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D28S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D280","SFP28","DWDM/100GHz","Fiber-pair","SM","D9280","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D29S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D290","SFP28","DWDM/100GHz","Fiber-pair","SM","D9290","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D30S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D300","SFP28","DWDM/100GHz","Fiber-pair","SM","D9300","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D31S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D310","SFP28","DWDM/100GHz","Fiber-pair","SM","D9310","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D32S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D320","SFP28","DWDM/100GHz","Fiber-pair","SM","D9320","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D33S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D330","SFP28","DWDM/100GHz","Fiber-pair","SM","D9330","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D34S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D340","SFP28","DWDM/100GHz","Fiber-pair","SM","D9340","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D35S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D350","SFP28","DWDM/100GHz","Fiber-pair","SM","D9350","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D36S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D360","SFP28","DWDM/100GHz","Fiber-pair","SM","D9360","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D37S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D370","SFP28","DWDM/100GHz","Fiber-pair","SM","D9370","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D38S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D380","SFP28","DWDM/100GHz","Fiber-pair","SM","D9380","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D39S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D390","SFP28","DWDM/100GHz","Fiber-pair","SM","D9390","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D40S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D400","SFP28","DWDM/100GHz","Fiber-pair","SM","D9400","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D41S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D410","SFP28","DWDM/100GHz","Fiber-pair","SM","D9410","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D42S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D420","SFP28","DWDM/100GHz","Fiber-pair","SM","D9420","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D43S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D430","SFP28","DWDM/100GHz","Fiber-pair","SM","D9430","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D44S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D440","SFP28","DWDM/100GHz","Fiber-pair","SM","D9440","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D45S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D450","SFP28","DWDM/100GHz","Fiber-pair","SM","D9450","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D46S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D460","SFP28","DWDM/100GHz","Fiber-pair","SM","D9460","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D47S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D470","SFP28","DWDM/100GHz","Fiber-pair","SM","D9470","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D48S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D480","SFP28","DWDM/100GHz","Fiber-pair","SM","D9480","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D49S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D490","SFP28","DWDM/100GHz","Fiber-pair","SM","D9490","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D50S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D500","SFP28","DWDM/100GHz","Fiber-pair","SM","D9500","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D51S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D510","SFP28","DWDM/100GHz","Fiber-pair","SM","D9510","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D52S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D520","SFP28","DWDM/100GHz","Fiber-pair","SM","D9520","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D53S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D530","SFP28","DWDM/100GHz","Fiber-pair","SM","D9530","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D54S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D540","SFP28","DWDM/100GHz","Fiber-pair","SM","D9540","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D55S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D550","SFP28","DWDM/100GHz","Fiber-pair","SM","D9550","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D56S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D560","SFP28","DWDM/100GHz","Fiber-pair","SM","D9560","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D57S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D570","SFP28","DWDM/100GHz","Fiber-pair","SM","D9570","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D58S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D580","SFP28","DWDM/100GHz","Fiber-pair","SM","D9580","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D59S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D590","SFP28","DWDM/100GHz","Fiber-pair","SM","D9590","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"32G-IR-D60S-BR","SFP28, 32/16/8G FC, Secure Optics Transceiver, DWDM 100GHz grid, 10km, 7dB, LC, D600","SFP28","DWDM/100GHz","Fiber-pair","SM","D9600","32G_FC/16G FC/8G FC","10km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D20S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D200","SFP+","DWDM/100GHz","Fiber-pair","SM","D9200","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D21S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D210","SFP+","DWDM/100GHz","Fiber-pair","SM","D9210","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D22S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D220","SFP+","DWDM/100GHz","Fiber-pair","SM","D9220","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D23S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D230","SFP+","DWDM/100GHz","Fiber-pair","SM","D9230","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D24S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D240","SFP+","DWDM/100GHz","Fiber-pair","SM","D9240","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D25S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D250","SFP+","DWDM/100GHz","Fiber-pair","SM","D9250","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D26S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D260","SFP+","DWDM/100GHz","Fiber-pair","SM","D9260","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D27S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D270","SFP+","DWDM/100GHz","Fiber-pair","SM","D9270","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D28S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D280","SFP+","DWDM/100GHz","Fiber-pair","SM","D9280","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D29S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D290","SFP+","DWDM/100GHz","Fiber-pair","SM","D9290","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D30S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D300","SFP+","DWDM/100GHz","Fiber-pair","SM","D9300","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D31S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D310","SFP+","DWDM/100GHz","Fiber-pair","SM","D9310","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D32S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D320","SFP+","DWDM/100GHz","Fiber-pair","SM","D9320","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D33S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D330","SFP+","DWDM/100GHz","Fiber-pair","SM","D9330","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D34S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D340","SFP+","DWDM/100GHz","Fiber-pair","SM","D9340","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D35S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D350","SFP+","DWDM/100GHz","Fiber-pair","SM","D9350","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D36S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D360","SFP+","DWDM/100GHz","Fiber-pair","SM","D9360","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D37S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D370","SFP+","DWDM/100GHz","Fiber-pair","SM","D9370","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D38S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D380","SFP+","DWDM/100GHz","Fiber-pair","SM","D9380","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D39S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D390","SFP+","DWDM/100GHz","Fiber-pair","SM","D9390","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D40S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D400","SFP+","DWDM/100GHz","Fiber-pair","SM","D9400","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D41S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D410","SFP+","DWDM/100GHz","Fiber-pair","SM","D9410","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D42S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D420","SFP+","DWDM/100GHz","Fiber-pair","SM","D9420","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D43S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D430","SFP+","DWDM/100GHz","Fiber-pair","SM","D9430","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D44S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D440","SFP+","DWDM/100GHz","Fiber-pair","SM","D9440","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D45S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D450","SFP+","DWDM/100GHz","Fiber-pair","SM","D9450","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D46S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D460","SFP+","DWDM/100GHz","Fiber-pair","SM","D9460","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D47S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D470","SFP+","DWDM/100GHz","Fiber-pair","SM","D9470","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D48S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D480","SFP+","DWDM/100GHz","Fiber-pair","SM","D9480","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D49S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D490","SFP+","DWDM/100GHz","Fiber-pair","SM","D9490","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D50S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D500","SFP+","DWDM/100GHz","Fiber-pair","SM","D9500","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D51S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D510","SFP+","DWDM/100GHz","Fiber-pair","SM","D9510","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D52S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D520","SFP+","DWDM/100GHz","Fiber-pair","SM","D9520","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D53S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D530","SFP+","DWDM/100GHz","Fiber-pair","SM","D9530","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D54S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D540","SFP+","DWDM/100GHz","Fiber-pair","SM","D9540","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D55S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D550","SFP+","DWDM/100GHz","Fiber-pair","SM","D9550","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D56S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D560","SFP+","DWDM/100GHz","Fiber-pair","SM","D9560","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D57S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D570","SFP+","DWDM/100GHz","Fiber-pair","SM","D9570","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D58S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D580","SFP+","DWDM/100GHz","Fiber-pair","SM","D9580","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D59S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D590","SFP+","DWDM/100GHz","Fiber-pair","SM","D9590","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"16G-ER-D60S-BR2","SFP+ 16G/8/4G FC, Secure Optics Transceiver, DWDM 100GHz grid, 40km, 14dB, LC, D600","SFP+","DWDM/100GHz","Fiber-pair","SM","D9600","16G FC/8G FC/4G FC","40km","Brocade","C-temp","Datasheet"]
[null,"SO-SFP28-32GFC-LR10-C27","SFP28, 32G FC, 25G/10G Ethernet, CWDM, 10km, 9.4dB, LC, 1270nm","SFP28","CWDM","Fiber-pair","SM","1270nm","32G_FC/25GE/10GbE-LAN","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP28-32GFC-LR10-C29","SFP28, 32G FC, 25G/10G Ethernet, CWDM, 10km, 9.4dB, LC, 12790nm","SFP28","CWDM","Fiber-pair","SM","1290nm","32G_FC/25GE/10GbE-LAN","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP28-32GFC-LR10-C31","SFP28, 32G FC, 25G/10G Ethernet, CWDM, 10km, 9.4dB, LC, 1310nm","SFP28","CWDM","Fiber-pair","SM","1310nm","32G_FC/25GE/10GbE-LAN","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP28-32GFC-LR10-C33","SFP28, 32G FC, 25G/10G Ethernet, CWDM, 10km, 9.4dB, LC, 1330nm","SFP28","CWDM","Fiber-pair","SM","1330nm","32G_FC/25GE/10GbE-LAN","10km",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC1M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 1m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","1m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC2M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 2m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","2m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC3M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 3m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","3m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC4M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 4m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","4m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC5M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 5m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","5m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC6M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 6m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","6m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC7M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 7m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","7m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC8M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 8m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","8m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC9M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 9m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","9m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC10M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 10m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","10m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC12M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 12m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","12m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC15M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 15m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","15m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC20M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 20m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","20m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-AOC30M","SFP28 to SFP28 Active Optical Cable (AOC), 25G Ethernet, 30m","SFP28","AOC","Fiber-pair","MM","850nm","25GE","30m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-BX10D-2733-I","SFP28, BiDi, 25G Ethernet, CPRI Opt10, Tx/Rx=1270/1330nm, 10km, 11dB, I-tmp, LC","SFP28","BiDi","Single-fiber","SM","1270/1330nm","25GE/CPRI-10","10km",null,"I-temp","Datasheet"]
[null,"SO-SFP28-BX10D-3327-I","SFP28, BiDi, 25G Ethernet, CPRI Opt10, Tx/Rx=1330/1270nm, 10km, 11dB, I-tmp, LC","SFP28","BiDi","Single-fiber","SM","1330/1270nm","25GE/CPRI-10","10km",null,"I-temp","Datasheet"]
[null,"SO-SFP28-BX20D-2733-I","SFP28, BiDi, 25G Ethernet, CPRI Opt10, Tx/Rx=1270/1330nm, 20km, 14.5dB, I-tmp, LC","SFP28","BiDi","Single-fiber","SM","1270/1330nm","25GE/CPRI-10","20km",null,"I-temp","Datasheet"]
[null,"SO-SFP28-BX20D-3327-I","SFP28, BiDi, 25G Ethernet, CPRI Opt10, Tx/Rx=1330/1270nm, 20km, 14.5dB, I-tmp, LC","SFP28","BiDi","Single-fiber","SM","1330/1270nm","25GE/CPRI-10","20km",null,"I-temp","Datasheet"]
[null,"SO-SFP28-BX40D-2731-I","SFP28, BiDi, 25G Ethernet, CPRI Opt10, Tx/Rx=1270/1310nm, 40km, 18dB, I-tmp, LC","SFP28","BiDi","Single-fiber","SM","1270/1310nm","25GE/CPRI-10","40km",null,"I-temp","Datasheet"]
[null,"SO-SFP28-BX40D-3127-I","SFP28, BiDi, 25G Ethernet, CPRI Opt10, Tx/Rx=1310/1270nm, 40km, 18dB, I-tmp, LC","SFP28","BiDi","Single-fiber","SM","1310/1270nm","25GE/CPRI-10","40km",null,"I-temp","Datasheet"]
[null,"SO-SFP28-LR","SFP28, 25G/10G Ethernet LR, 1310nm, SM, 10km, 6.3dB, LC","SFP28","Grey","Fiber-pair","SM","1310nm","25GE/CPRI-10/10GbE-LAN","10km","25GBASE-LR","C-temp","Datasheet"]
[null,"SO-QSFP28-PCU0.5M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 0.5m, passive","QSFP28","DAC","Coax","Electrical","-","25GE","0.5m",null,"C-temp","Datasheet"]
[null,"SO-QSFP28-PCU1M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 1m, passive","QSFP28","DAC","Coax","Electrical","-","25GE","1m",null,"C-temp","Datasheet"]
[null,"SO-QSFP28-PCU2M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 2m, passive","QSFP28","DAC","Coax","Electrical","-","25GE","2m",null,"C-temp","Datasheet"]
[null,"SO-QSFP28-PCU3M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG30, 3m, passive","QSFP28","DAC","Coax","Electrical","-","25GE","3m",null,"C-temp","Datasheet"]
[null,"SO-QSFP28-PCU5M","QSFP28 to QSFP28 Direct Attach Cable (DAC), 100G Ethernet, AWG26, 5m, passive","QSFP28","DAC","Coax","Electrical","-","25GE","5m",null,"C-temp","Datasheet"]
[null,"SO-SFP28-SR","SFP28, 25G Ethernet SR, MM 850nm, 100m, 1.9dB, LC","SFP28","Grey","Fiber-pair","MM","850nm","25GE","100m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-SFP28-ER-I","SFP28, 25G/10G Ethernet LR, 1310nm, SM, 40km, 18dB, LC, I-temp","SFP28","Grey","Fiber-pair","SM","1310nm","25GE","40km","25GBASE-ER","I-temp","Datasheet"]
[null,"SO-SFP28-SR3","SFP28, 25G Ethernet, 850nm, MM, DDM, 1.9dB, 200m@OM3, 300m@OM4, LC","SFP28","Grey","Fiber-pair","MM","850nm","25GE","300m","25GBASE-SR","C-temp","Datasheet"]
[null,"SO-TXFP-10G-ZR-DWDM-A","XFP, 10G Multirate 9.95-11.35Gbps, DWDM 50GHz Tunable, 191.35 - 196.10 THz (96ch), 80km, 25dB, LC","XFP","DWDM/50GHz-Tune","Fiber-pair","SM","D9135 - D9610","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-10GE-BX10D-2733","XFP, BiDi, 10G Multirate 9.95-11.1Gbps, Tx/Rx=1270/1330nm, 10km, 9dB, LC","XFP","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-10GE-BX10D-3327","XFP, BiDi, 10G Multirate 9.95-11.1Gbps, Tx/Rx=1330/1270nm, 10km, 9dB, LC","XFP","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-10GE-BX20D-2733","XFP, BiDi, 10G Multirate 9.95-11.1Gbps, Tx/Rx=1270/1330nm, 20km, 12dB, LC","XFP","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","20km",null,"C-temp","Datasheet"]
[null,"SO-XFP-10GE-BX20D-3327","XFP, BiDi, 10G Multirate 9.95-11.1Gbps, Tx/Rx=1330/1270nm, 20km, 12dB, LC","XFP","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","20km",null,"C-temp","Datasheet"]
[null,"SO-XFP-10GE-BX40D-2733","XFP, BiDi, 10G Multirate 9.95-11.1Gbps, Tx/Rx=1270/1330nm, 40km, 16dB, LC","XFP","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-10GE-BX40D-3327","XFP, BiDi, 10G Multirate 9.95-11.1Gbps, Tx/Rx=1330/1270nm, 40km, 16dB, LC","XFP","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-10GE-BX60D-2733","XFP, BiDi, 10G Multirate 9.95-11.1Gbps, Tx/Rx=1270/1330nm, 60km, 21dB, LC","XFP","BiDi","Single-fiber","SM","1270/1330nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","60km",null,"C-temp","Datasheet"]
[null,"SO-XFP-10GE-BX60D-3327","XFP, BiDi, 10G Multirate 9.95-11.1Gbps, Tx/Rx=1330/1270nm, 60km, 21dB, LC","XFP","BiDi","Single-fiber","SM","1330/1270nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","60km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER","XFP, 10G Multirate 8.5-11.1Gbps, SM, 1550nm, 40km, 16dB, LC","XFP","Grey","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/8G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-C47","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 40km, 14dB, LC, 1470nm","XFP","CWDM","Fiber-pair","SM","1470nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-C49","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 40km, 14dB, LC, 1490nm","XFP","CWDM","Fiber-pair","SM","1490nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-C51","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 40km, 14dB, LC, 1510nm","XFP","CWDM","Fiber-pair","SM","1510nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-C53","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 40km, 14dB, LC, 1530nm","XFP","CWDM","Fiber-pair","SM","1530nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-C55","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 40km, 14dB, LC, 1550nm","XFP","CWDM","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-C57","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 40km, 14dB, LC, 1570nm","XFP","CWDM","Fiber-pair","SM","1570nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-C59","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 40km, 14dB, LC, 1590nm","XFP","CWDM","Fiber-pair","SM","1590nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-C61","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 40km, 14dB, LC, 1610nm","XFP","CWDM","Fiber-pair","SM","1610nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9190","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9190","XFP","DWDM/100GHz","Fiber-pair","SM","D9190","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9200","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9200","XFP","DWDM/100GHz","Fiber-pair","SM","D9200","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9210","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9210","XFP","DWDM/100GHz","Fiber-pair","SM","D9210","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9220","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9220","XFP","DWDM/100GHz","Fiber-pair","SM","D9220","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9230","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9230","XFP","DWDM/100GHz","Fiber-pair","SM","D9230","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9240","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9240","XFP","DWDM/100GHz","Fiber-pair","SM","D9240","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9250","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9250","XFP","DWDM/100GHz","Fiber-pair","SM","D9250","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9260","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9260","XFP","DWDM/100GHz","Fiber-pair","SM","D9260","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9270","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9270","XFP","DWDM/100GHz","Fiber-pair","SM","D9270","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9280","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9280","XFP","DWDM/100GHz","Fiber-pair","SM","D9280","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9290","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9290","XFP","DWDM/100GHz","Fiber-pair","SM","D9290","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9300","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9300","XFP","DWDM/100GHz","Fiber-pair","SM","D9300","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9310","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9310","XFP","DWDM/100GHz","Fiber-pair","SM","D9310","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9320","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9320","XFP","DWDM/100GHz","Fiber-pair","SM","D9320","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9330","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9330","XFP","DWDM/100GHz","Fiber-pair","SM","D9330","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9340","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9340","XFP","DWDM/100GHz","Fiber-pair","SM","D9340","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9350","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9350","XFP","DWDM/100GHz","Fiber-pair","SM","D9350","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9360","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9360","XFP","DWDM/100GHz","Fiber-pair","SM","D9360","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9370","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9370","XFP","DWDM/100GHz","Fiber-pair","SM","D9370","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9380","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9380","XFP","DWDM/100GHz","Fiber-pair","SM","D9380","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9390","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9390","XFP","DWDM/100GHz","Fiber-pair","SM","D9390","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9400","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9400","XFP","DWDM/100GHz","Fiber-pair","SM","D9400","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9410","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9410","XFP","DWDM/100GHz","Fiber-pair","SM","D9410","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9420","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9420","XFP","DWDM/100GHz","Fiber-pair","SM","D9420","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9430","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9430","XFP","DWDM/100GHz","Fiber-pair","SM","D9430","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9440","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9440","XFP","DWDM/100GHz","Fiber-pair","SM","D9440","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9450","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9450","XFP","DWDM/100GHz","Fiber-pair","SM","D9450","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9460","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9460","XFP","DWDM/100GHz","Fiber-pair","SM","D9460","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9470","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9470","XFP","DWDM/100GHz","Fiber-pair","SM","D9470","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9480","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9480","XFP","DWDM/100GHz","Fiber-pair","SM","D9480","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9490","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9490","XFP","DWDM/100GHz","Fiber-pair","SM","D9490","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9500","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9500","XFP","DWDM/100GHz","Fiber-pair","SM","D9500","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9510","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9510","XFP","DWDM/100GHz","Fiber-pair","SM","D9510","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9520","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9520","XFP","DWDM/100GHz","Fiber-pair","SM","D9520","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9530","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9530","XFP","DWDM/100GHz","Fiber-pair","SM","D9530","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9540","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9540","XFP","DWDM/100GHz","Fiber-pair","SM","D9540","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9550","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9550","XFP","DWDM/100GHz","Fiber-pair","SM","D9550","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9560","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9560","XFP","DWDM/100GHz","Fiber-pair","SM","D9560","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9570","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9570","XFP","DWDM/100GHz","Fiber-pair","SM","D9570","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9580","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9580","XFP","DWDM/100GHz","Fiber-pair","SM","D9580","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9590","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9590","XFP","DWDM/100GHz","Fiber-pair","SM","D9590","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-D9600","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 40km, 14dBm, LC, D9600","XFP","DWDM/100GHz","Fiber-pair","SM","D9600","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ER-I","XFP, 10G Multirate 8.5-11.1Gbps, SM, 1550nm, 40km, 16dB, I-temp, LC","XFP","Grey","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/8G FC/OTU2/OTU2e/CPRI8","40km",null,"I-temp","Datasheet"]
[null,"SO-XFP-LR","XFP, 10G Multirate 9.95-11.1Gbps, SM, 1310nm, 10km, 8.5dB, LC","XFP","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km","10GBASE-LR","C-temp","Datasheet"]
[null,"SO-XFP-LR20","XFP, 10G Multirate 9.95-11.1Gbps, SM, 1310nm, 20km, 12dB, LC","XFP","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","20km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR40","XFP, 10G Multirate 9.95-11.1Gbps, SM, 1310nm, 40km, 16dB, LC","XFP","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","40km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C27","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1270nm","XFP","CWDM","Fiber-pair","SM","1270nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C29","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1290nm","XFP","CWDM","Fiber-pair","SM","1290nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C31","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1310nm","XFP","CWDM","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C33","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1330nm","XFP","CWDM","Fiber-pair","SM","1330nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C35","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1350nm","XFP","CWDM","Fiber-pair","SM","1350nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C37","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1370nm","XFP","CWDM","Fiber-pair","SM","1370nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C39","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1390nm","XFP","CWDM","Fiber-pair","SM","1390nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C41","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1410nm","XFP","CWDM","Fiber-pair","SM","1410nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C43","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1430nm","XFP","CWDM","Fiber-pair","SM","1430nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C45","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1450nm","XFP","CWDM","Fiber-pair","SM","1450nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C47","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1470nm","XFP","CWDM","Fiber-pair","SM","1470nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C49","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1490nm","XFP","CWDM","Fiber-pair","SM","1490nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C51","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1510nm","XFP","CWDM","Fiber-pair","SM","1510nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C53","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1530nm","XFP","CWDM","Fiber-pair","SM","1530nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C55","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1550nm","XFP","CWDM","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C57","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1570nm","XFP","CWDM","Fiber-pair","SM","1570nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C59","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1590nm","XFP","CWDM","Fiber-pair","SM","1590nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-C61","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 10km, 10dB, LC, 1610nm","XFP","CWDM","Fiber-pair","SM","1610nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km",null,"C-temp","Datasheet"]
[null,"SO-XFP-LR-I","XFP, 10G Multirate 9.95-11.1Gbps, SM, 1310nm, 10km, 8.5dB, I-temp, LC","XFP","Grey","Fiber-pair","SM","1310nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","10km","10GBASE-LR","I-temp","Datasheet"]
[null,"SO-XFP-LRM","XFP, 10G Ethernet  LRM, 1310nm, MM, 1310nm, 300m@OM3, 2dB, LC","XFP","Grey","Fiber-pair","MM","1310nm","10GbE-LAN","300m",null,"C-temp","Datasheet"]
[null,"SO-XFP-SR","XFP, 10G Multirate 9.95-11.3Gbps, MM, 850nm, 300m@OM3, 3.8dB, LC","XFP","Grey","Fiber-pair","MM","850nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","300m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-XFP-SR-E","XFP, 10G Multirate 9.95-11.3Gbps, MM, 850nm, 300m@OM3, 3.8dB, E-temp, LC","XFP","Grey","Fiber-pair","MM","850nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","300m","10GBASE-SR","C-temp","Datasheet"]
[null,"SO-XFP-ZR","XFP, 10G Multirate 9.95-11.3Gbps, SM, 1550nm, 80km, 24dB, LC","XFP","Grey","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-C47","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 80km, 24dB, LC, 1470nm","XFP","CWDM","Fiber-pair","SM","1470nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-C49","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 80km, 24dB, LC, 1490nm","XFP","CWDM","Fiber-pair","SM","1490nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-C51","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 80km, 24dB, LC, 1510nm","XFP","CWDM","Fiber-pair","SM","1510nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-C53","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 80km, 24dB, LC, 1530nm","XFP","CWDM","Fiber-pair","SM","1530nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-C55","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 80km, 24dB, LC, 1550nm","XFP","CWDM","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-C57","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 80km, 24dB, LC, 1570nm","XFP","CWDM","Fiber-pair","SM","1570nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-C59","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 80km, 24dB, LC, 1590nm","XFP","CWDM","Fiber-pair","SM","1590nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-C61","XFP, 10G Multirate 9.95-11.1Gbps, CWDM, 80km, 24dB, LC, 1610nm","XFP","CWDM","Fiber-pair","SM","1610nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9190","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9190","XFP","DWDM/100GHz","Fiber-pair","SM","D9190","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9200","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9200","XFP","DWDM/100GHz","Fiber-pair","SM","D9200","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9210","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9210","XFP","DWDM/100GHz","Fiber-pair","SM","D9210","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9220","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9220","XFP","DWDM/100GHz","Fiber-pair","SM","D9220","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9230","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9230","XFP","DWDM/100GHz","Fiber-pair","SM","D9230","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9240","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9240","XFP","DWDM/100GHz","Fiber-pair","SM","D9240","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9250","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9250","XFP","DWDM/100GHz","Fiber-pair","SM","D9250","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9260","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9260","XFP","DWDM/100GHz","Fiber-pair","SM","D9260","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9270","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9270","XFP","DWDM/100GHz","Fiber-pair","SM","D9270","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9280","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9280","XFP","DWDM/100GHz","Fiber-pair","SM","D9280","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9290","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9290","XFP","DWDM/100GHz","Fiber-pair","SM","D9290","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9300","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9300","XFP","DWDM/100GHz","Fiber-pair","SM","D9300","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9310","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9310","XFP","DWDM/100GHz","Fiber-pair","SM","D9310","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9320","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9320","XFP","DWDM/100GHz","Fiber-pair","SM","D9320","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9330","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9330","XFP","DWDM/100GHz","Fiber-pair","SM","D9330","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9340","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9340","XFP","DWDM/100GHz","Fiber-pair","SM","D9340","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9350","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9350","XFP","DWDM/100GHz","Fiber-pair","SM","D9350","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9360","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9360","XFP","DWDM/100GHz","Fiber-pair","SM","D9360","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9370","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9370","XFP","DWDM/100GHz","Fiber-pair","SM","D9370","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9380","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9380","XFP","DWDM/100GHz","Fiber-pair","SM","D9380","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9390","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9390","XFP","DWDM/100GHz","Fiber-pair","SM","D9390","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9400","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9400","XFP","DWDM/100GHz","Fiber-pair","SM","D9400","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9410","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9410","XFP","DWDM/100GHz","Fiber-pair","SM","D9410","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9420","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9420","XFP","DWDM/100GHz","Fiber-pair","SM","D9420","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9430","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9430","XFP","DWDM/100GHz","Fiber-pair","SM","D9430","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9440","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9440","XFP","DWDM/100GHz","Fiber-pair","SM","D9440","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9450","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9450","XFP","DWDM/100GHz","Fiber-pair","SM","D9450","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9460","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9460","XFP","DWDM/100GHz","Fiber-pair","SM","D9460","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9470","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9470","XFP","DWDM/100GHz","Fiber-pair","SM","D9470","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9480","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9480","XFP","DWDM/100GHz","Fiber-pair","SM","D9480","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9490","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9490","XFP","DWDM/100GHz","Fiber-pair","SM","D9490","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9500","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9500","XFP","DWDM/100GHz","Fiber-pair","SM","D9500","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9510","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9510","XFP","DWDM/100GHz","Fiber-pair","SM","D9510","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9520","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9520","XFP","DWDM/100GHz","Fiber-pair","SM","D9520","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9530","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9530","XFP","DWDM/100GHz","Fiber-pair","SM","D9530","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9540","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9540","XFP","DWDM/100GHz","Fiber-pair","SM","D9540","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9550","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9550","XFP","DWDM/100GHz","Fiber-pair","SM","D9550","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9560","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9560","XFP","DWDM/100GHz","Fiber-pair","SM","D9560","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9570","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9570","XFP","DWDM/100GHz","Fiber-pair","SM","D9570","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9580","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9580","XFP","DWDM/100GHz","Fiber-pair","SM","D9580","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9590","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9590","XFP","DWDM/100GHz","Fiber-pair","SM","D9590","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-D9600","XFP, 10G Multirate 9.95-11.1Gbps, DWDM 100GHz, 80km, 24dBm, LC, D9600","XFP","DWDM/100GHz","Fiber-pair","SM","D9600","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"C-temp","Datasheet"]
[null,"SO-XFP-ZR-I","XFP, 10G Multirate 9.95-11.3Gbps, SM, 1550nm, 80km, 24dB, I-temp, LC","XFP","Grey","Fiber-pair","SM","1550nm","10GbE-LAN/10GbE-WAN/STM-64/OC-192/10G FC/OTU2/OTU2e/CPRI8","80km",null,"I-temp","Datasheet"]